VP Subject List
Subject
ADAPTERS	ADHESIVES / SEALANTS	AIR	ANTI-STATIC
ASTRAGALS	BABBITTS	BAGS	BANDS
BARRICADES	BATTERIES / CHARGERS	BATTERY CHARGERS	BATTERY TESTERS
BEARINGS	BELLS	BELTS	BINDERS
BLADES	BLOWERS	BOLTS	BOOTS
BOXES	BRACKETS	BRAILLE FIXTURES	BRAKES
BROOMS	BRUSH HOLDERS	BRUSHES	BUCKETS
BUMPERS	BUSHINGS	BUTTONS	BUZZERS
CABINETS	CABLE BANDS	CABLE TIES	CABLES / CORDS
CAPACITORS	CAPS, BEARING	CAPS, BRUSH	CAPS, FRICTION
CARD CAGES	CARS	CARTONS	CASTINGS
CHAINS	CLAMPS / CLIPS	CLEANERS	CLIPBOARD
CLIPS	CLOSERS	CLOTH	CLOTH, FIBERGLASS
COILS	CONNECTORS	CONTACTS	COUPLINGS
COVERS	CROSS SLIDE	DASHPOTS	DECALS
DEVICES	DIODES	DISKS, COMPUTER	DOOR CHECKS
DOOR LOCKS	DOOR OPERATORS	DOOR SILENCERS	DRILLS
EMERY CLOTH	ENCODERS	EPROMS	FASTENERS
FELT	FILES	FILTERS	FIRST AID
FLAGS	FLASHLIGHT	FUSEHOLDERS	FUSES
GAL	GASKETS	GAUGES	GEAR REDUCT.UNITS
GEARS	GIBS/GUIDES	GLOVES	GREASE GUNS
GRILLS	GROMMETS	GUARDS	HARDWARE CLOTH
HEATERS	HINGES	HOSES	HOUSINGS
INK	INSERTS	INSULATORS	JEWELS
KEYS	KITS	LABELS	LAMPS
LEAFLET MICROFICHE	LEAFLETS	LIGHT FIXTURES	LINERS
LININGS	LINKS	LOCKBOX	LOCKS
LUBRICANTS	LUBRICATORS	MANUALS	MARKERS
MATS	METERS	MICROFICHE	MODULATORS
MODULES	MOPS	MOTORS	MRVF
NEEDLES	NUTS	OILCANS	ORANGE STICKS
P.C. BOARDS	PACKING	PADS	PAILS
PAINTS	PANELS	PANS	PAPER
PINS	PIPE PLUGS	PLANKS	PLASTIC SHEETS

Subject				
PLATES	PLIERS	PLUGS	PLUNGERS	
POWER SUPPLIES	PULL STRAPS	PUMPS	RECTIFIERS	
REELS	REGULATORS	RELAYS	RESISTORS	
RESPIRATORS	RESPIRATORS, FILTERS	RINGS	RODS	
ROLLERS	ROPES	SAFETY NETTING	SAFETY SUPPLIES	
SAFETY SUPPLIES, FIRE	SAFETY SUPPLIES, LABELS	SAFETY SUPPLIES, SIGNS	SAFETY SUPPLIES, SPILL	
SAFETY SUPPLIES, UNIFORM	SCREWS	SEALS	SES	
SHAFTS	SHAPES	SHIMS	SHOES	
SIGNS	SLATS	SLEEVING	SOCKETS	
SOLDERS	SPACERS	SPLICERS	SPRAYERS	
SPRINGS	SPROCKETS	STANDOFFS	STAPLE REMOVER	
STARTERS	STATORS	STEP PIN LIFTER	STONES	
STRAPS	STRIKERS	SUPPRESSORS	SWITCHES	
TAGS	TAPES	TAPS	TARGETS	
TERMINAL STRIPS	TERMINALS	TESTERS	THERMISTORS	
THERMOSTATS	TIGHTENERS	TIMERS	TOOL BOXES	
TORQUE MULTIPLIERS	TRANSFORMERS	TUBES	TUBING	
TY-RAPS	VALVES	VANES	WASHERS	
WEDGE GUARDS	WEDGE GUARDS	WHEELS	WICKS	
WIPERS	WIRES	WIRING DIAGRAMS	WORMS	
WRENCHES				

	Page 1

Subject	VP#	Description
ADHESIVES / SEALANTS ADHESIVES / SEALANTS
VP-420455	Primer N 7649. In a 4.5 ounce aerosol can. Use to
speed the cure of Loctite Threadlocker products (242, 262, etc.) and to ensure proper cure on inactive metals.
VP-700100	Adhesive & sealant kit containing following: VP‑
700105, VP-700110, VP-700115, VP-700121, VP-700130, VP-700135, VP-700140, VP-420455. 
VP-700105	RTV Silicone Gasket Maker: Loctite 587 in 70 ml
tubes. 
VP-700110	Threadlocker: Loctite 242 in 0.34 fl.oz. Bottle.
Medium strength threadlocker for parts between 1/4" and 3/4" diameter. Removable with hand tools. 
VP-700112	Threadlocker: Loctite Threadlocker 222. In 10ml
Bottle, for locking all fasteners 1/4" dia. or smaller. Removable with hand tools.
VP-700117	Threadlocker: Loctite 271 in 10ml (0.34 fl.oz)
bottle. High-strength threadlocking for parts up to 1 inch diameter. Also used in Hollister Whitney Disc Brake Upgrade kit 
VP-700120	Retaining Compound: Loctite 609 Sleeve & Bearing
Mount, in 10ml bottle. Secures bearings, bushings. Restores fit to bearings, etc. 
VP-700121	Retaining Compound: Loctite 660 Quick Metal®
Retaining Compound Press Fit Repair, in 6ml bottle. Fills gap to 0.02" diameter clearance. Restores correct fit to matching assemblies.
VP-700122	Retaining Compound 648 high strength/rapid cure,
10ml bottle. Fills gaps up to 0.006” diameter clearance. Fixtures in 5 min.

	Page 2

Subject	VP#	Description
ADHESIVES / SEALANTS
VP-700123	Retaining Compound: Loctite 638, in 10 ml bottle.
High strength/quick fixturing retaining compound for loose fitting parts. Fills gaps up to .015" diameter clearance. Fixtures in 5 min.
VP-700125	Casting Sealant: Loctite 290, in 0.34 fl.oz bottle.
      Seals porosities in castings & welds.
VP-700130	Gasket Eliminator Sealant: Loctite 518, in 50 ml
tube. A form-in-place gasketing compound, flexes w/movement. 
VP-700135	Pipe Thread Sealant: Loctite 565 PST® Pipe Sealant
in 50ml tube. Seals threaded metal pipe fittings, prevents leakage. 
VP-700139	Instant Adhesive: Loctite 416, in 1oz. tube. Bonds
rough/irregular surfaces. Align times less than 15 sec. For use in adhering tension frame gibs. 
VP-700140	Instant Adhesive: Loctite PRISM® 454, in 3-gram
tube. General purpose, no-run clear gel. Ideal for porous substrates/rough/acidic surfaces. 
VP-700145	Epoxy: Fixmaster® Fast cure Epoxy Mixing Cups.
One can containing ten 4-gram handy mixing cups. 5 minute working time. Full cure in 12 hrs. 
VP-700150	Otis/Loctite adhesives & sealant application guide
slide rule. 
VP-700160	High Strength Acrylic Adhesive Kit: Kit of Loctite
Speedbonder #324 (VP-700161) and Activator #7075 (VP-700162).
VP-700161	High Strength Acrylic Adhesive: Loctite
Speedbonder #324, in 50 ml. bottle. For use with VP-700162 and contained in kit VP-700160.
VP-700162	Adhesive Activator: Loctite Activator 7075, in 4.5
fl. oz. Spray Can. For use with VP-700161 and contained in kit VP-700160.

	Page 3

Subject	VP#	Description
ADHESIVES / SEALANTS
VP-700170	Tamper evident sealant. In 2 ounce bottle with
applicator brush in cap, white liquid. Used to seal adjustments on 7063 governor after calibration. 
VP-700175	Epoxy: Plastic Steel® 5-Minute Epoxy Putty (SF)
10240. (Devcon) in 1lb box. Dependible
emergency repairs in less than one hour. Cures above 40 degrees F.
VP-700400	Scotch grip adhesive, 3M Co.#2141, in 1-qt.can.
Used to glue brake linings of 155 machines per TA-111-5-14 & to hold coupling bushings of 22 & 29CT machines.
VP-700410	Bonding adhesive for sheave inserts 215BT &
215BV. In 1/2-oz. tubes w/6 month shelf life.
Humidity sensitive, 4 to 5 splices per tube.	
VP-734500	Rubber and Gasket Adhesive. 3M EC-847 in 5-oz.
tubes. 
VP-796000	Jewel resin epoxy kit.Contains (2) 50ml cartridges
of Loctite E-20HP plus dispenser kit to use in standard caulking gun. For engraved faceplates with poured jewels. Translucent White epoxy.
VP-804165	Joint sealant in 1.3 oz. tubes. Highside Chemicals
"LEAKLOCK". Seals oil leaks on hydro pump units & also gear case leaks. Apply to bolt, fitting threads, or to gaskets on cover plates.
VP-865861	Silicone sealant: GE 108 RTV in 2.5 oz. tubes. 
AIR
VP-700300	Canned air, 10-oz. can. Micro BlastTM Used in
MRVF Maintenance Tool Kit, VP-789700.
ANTI-STATIC
VP-700800	Anti-static kit. Velostat portable field service
grounding kit. 3M part #8012.
VP-700801	Speidel adjustable wrist strap. Comes complete
with 6 ft. coiled cord with built-in 1M ohm resistor, 4mm banana plug & alligator clip. U.L. listed.
VP-798901	Antistatic bag, opaque, heat sealable,
moisture/vapor proof. 
ASTRAGALS
VP-702420	Astragal, Dahlstrom Part #SPOSP924, 86" long.
VP-702430	Astragal, ESI P/N 2L1075248000, 84" long.

	Page 4

Subject	VP#	Description
BABBITTS
VP-702650	Common babbitt #3, cable shackle babbitt.
VP-702900	Babbitt, tuftex, Rollite #77 nickel alloy. Otis Spec 2.
Used for babbitted bearings on
machines,governors, and sheaves. Medium load. Suitable for "geared" sheave shaft bearings.
BAGS
VP-798901	SEE ANTI-STATIC.
VP-798903	Roll of 125 natural color, 33 Gal. plastic bags. 33" x
40" heavy grade, 0.624 mil. thickness.
BANDS
VP-703170	SEE CABLE BANDS.
VP-703175	SEE CABLE BANDS.
VP-703180	SEE CABLE BANDS.
VP-703185	SEE CABLE BANDS.

BATTERIES
VP-703900	Brush on battery terminal compound. Used to
prevent corrosion of terminals on MRVF batteries. NCP-2 brush-on compound.
VP-703990	Battery for EPCO surface mounted emergency light
fixtures, VP-810220 & VP-810225. 6V gell cell battery. Power Sonic PS-626. 
VP-704130	Battery charger, Renewal Power Station2. Eight
position charger for AA, AAA, C, D Renewal batteries. Drop Ship item.
VP-704140	Battery/Charger Kit. Includes: (1) Renewal Power
Station2; (4) D size, (2) C size, (4) AA size, (4) AAA size Renewal batteries. Drop Ship item.
VP-704150	1.5 volt, button cell battery. Rayovac type 357.
Used in Circuit Alert Voltage Probe, p/n MT-122099-1.
VP-704174	AA size, Renewal Alkaline rechargeable battery
1.5V. Drop Ship item.
VP-704175	AA size battery.
VP-704179	AAA size, Renewal Alkaline rechargeable battery.
1.5V. Drop Ship item.
VP-704180	AAA size battery.

	Page5

Subject	VP#	Description
BATTERIES
VP-704185	9 Volt battery.
VP-704189	C size, Renewal Alkaline rechargeable battery.
1.5V. Drop Ship item.
VP-704190	C size battery.
VP-704199	D size, Renewal Alkaline rechargeable battery.
1.5V. Drop Ship item.
VP-704200	D size battery. Eveready Alkaline.
BEARINGS
VP-704375	Bearing, Torrington # B1616.
VP-704400	Cam follower, 5/8" O.D. Made by McGill,
Torrington Bearing, Smith Bearing Division, & RBC.
VP-704845	Pillowblock bearing. Consolidated # SY505D. SKF #
SY50FM (was # SY50FJ)
BELLS
VP-705700	Bell, Edwards Adaptabell #340-4E5. 4", 12 volt, 60
Hz, .62 amp., UL-Listed 116E.
VP-706050	Bell, 6-inch, 125 volts. W.L.Jenkins #2005.
BLADES
VP-706505	Hacksaw blade, Bi-Metal high speed steel. 18 teeth
per inch, 10 inches long.
VP-706550	Hacksaw blade, general purpose. 18 teeth per
inch, 12 inches long.
VP-706555	Hacksaw blade, Bi-Metal high speed steel. 18 teeth
per inch, 12 inches long.

	Page 6

Subject	VP#	Description
BLADES
VP-706605	Hacksaw blade, Bi-Metal high speed steel. 24 teeth
per inch, 10 inches long.
VP-706650	Hacksaw blade, general purpose. 24 teeth per
inch, 12 inches long.
VP-706655	Hacksaw blade, Bi-Metal high speed steel. 24 teeth
per inch, 12 inches long.
VP-706750	Hacksaw blade, general purpose. 32 teeth per
inch, 12 inches long.
VP-706755	Hacksaw blade, Bi-Metal high speed steel. 32 teeth
per inch, 12 inches long.
BOLTS
VP-709740	Hex head cap bolt, fully threaded. Din 933 M6 x 15
VP-709750	Hex head cap bolt, fully threaded. Din 933 M6 x 40
VP-709770	Hex head cap bolt, fully threaded. Din 933 M8 x 15
VP-709773	Hex head cap bolt, fully threaded. Din 933 M8 x 25
VP-709795	Hex head cap bolt, fully threaded. Din 933 M10 x
35.
VP-709820	Hex head cap bolt, fully threaded. Din 933 M12 x
60.
VP-709827	Hex head cap bolt, fully threaded. Din 933 M12 x
25.
VP-709833	Hex head cap bolt, fully threaded. Din 933 M12 x
50.
VP-709845	Hex head cap bolt, fully threaded. Din 933 M16 x
35.
VP-710650	Bolt J-10C. Weld screw w/butterfly nut; made
from Ohio Screw # HW2132 with a slot and a wing nut of size 1/4-20.
VP-711270	5/8" x 2" bolt, full thread; for 1/2 rail at World
Trade Center.
VP-711275	5/8" x 2-1/2" bolt, full thread; for 1/2 rail at World
Trade Center.
VP-711285	Finished hex head bolt, coarse thread. 3/8" x 1".

	Page 7

Subject	VP#	Description
BOLTS
VP-711287	3/8"-16 X 1-1/4" flanged, serrated hex head bolt,
full thread, zinc plated. For door track mounting on track/hanger kits.
VP-711290	3/8-16 x 1-1/2 hex bolt, full thread for door hanger
bolts.
VP-711295	1/2-13 x 1-1/2 hex bolt, full thread for door hanger
bolts.
VP-711300	Finished hex head bolt, NC 2A thread, brass. 5/8" x
2-1/2".
VP-711315	3/4" x 2-1/2" bolt, full thread; for World Trade
Center.
VP-711320	3/4" x 2" bolt, full thread; for 1/2 rail at World
Trade Center.
VP-711325	Finished hex head bolt, NC 2A thread, brass. 3/4" x
3".
VP-711326	Zinc plated hex head bolt, 3/4"-10 X 3-1/2". Full
thread, Grade 5. Used in MT-102050 pipe stands.
VP-712550	Machine bolt, 1/2" x 2-1/2".
VP-713350	Machine bolt, 5/8" x 1-1/2".
VP-713550	Hex head finish bolt 5/8" X 2-1/4". Grade 2.
VP-713555	Bolt for A288LJ lever. Modified 2" x 3/8" 16-cap
screw. 
VP-713700	Socket Flat Cap Screw 5/16-18 x 1/2 Zinc Plate
used to secure door-relating aircord with 386AKS1 plates.
VP-713705	Socket Flat Cap Screw 5/16-18 x 1/2 Black Oxide
used to secure door-relating aircord with 386AKS1 plates.
VP-804611	Steel spade bolts, zinc plated. Wenco # A-24A14-
1913. Part of VP-804615, Top-of-Car Insp. Light.
BOXES
VP-719470	Static protection box for shipping eproms and IC's.
Size: 3-3/4" x 3-3/4" x 1". Conductive Containers Inc.

	Page 8

Subject	VP#	Description
BRACKETS
VP-721550	Modified 316AHJ1 bracket for "F" Operator door
shoes. 
BRAKES
VP-722400	Brake equalizer for# 74, 74A, 74B gearless
Machines.
BROOMS
VP-722800	Corn broom for sweeping floor.
BRUSHES
VP-723466	Electro-graphitic brush for MRVF door motors.
Harder grade N1 motor brushes for screw type operators. 
VP-723516	Generator brush. GE #36A164452AAP6. Originally
used for generators (pre 1980) at Standard Oil in Chicago.
VP-724200	Radiator brush for dusting equipment.
VP-724210	Brush, Coated Steel Belt cleaning. Non-metallic,
firm bristle.
BUMPERS
VP-724810	Rubber bumper for Otis type 7040 interlock. 
VP-725350	Rubber bumper. Hoyt 3053, 1-1/8 D.F. 1-1/8"
diameter x 1/4" pad, 1/2" diameter x 1/2" long thd shank.
BUSHINGS
VP-725770	Bushing, Thompson catalog #10L10-F.
VP-725775	Bushing, Thompson catalog #8L3-1/2-F.
VP-725812	Bushing, Rulon part #0609-6. 3/8" x 9/16" x 3/4".
For use in A7063E governor.
BUTTONS
VP-728200	Aluminum Otis # A323AF1 button, unmarked.
VP-728210	Bullet nose aluminum button, vandal proof,
unmarked.

	Page 9

Subject	VP#	Description
BUTTONS
VP-728250	Brass Otis # A323AF1 button.
CABINETS
VP-729001	Maintenance cabinet. 42"H x 36"W x 18"D. Grey.
Grainger #4W280.
VP-729011	Maintenance cabinet. 72"H x 36"W x 18"D. Grey.
Grainger #4W278.
VP-729012	Hasp, for cabinets VP-729001 and VP-729011.
Grainger #6X700.
VP-729015	Cabinet, wall mounted. 30" long x 24" high x 13"
deep when closed. 60" long x 24" high x 6" deep when open. Grainger #2W178.
VP-729020	Cabinet, stand-up. 2.5 sq. ft. footprint.
Unassembled. Grainger #1W814.
VP-729021	Cabinet, stand-up. Assembled version of VP‑
729020
VP-846405	Safety storage cabinet (for gasoline and other
flammables & combustibles) 45 gal. capacity. Has 2 removable shelves. Cabinet external dimensions are 65" x 43" x 18".
CABLE BANDS
VP-703170	3/8" cable band, Morse Starrett. Used as seizing.
VP-703175	5/8" cable band, Morse Starrett. Used for seizing.
VP-703180	1/2" cable band, Morse Starrett. Used for seizing.
VP-703185	3/4" cable band, Morse Starrett. Used for seizing.
CABLE TIES
VP-897955	Cable tie with "Test & Verify" printed on tag.
Yellow, nylon, 5" long. 
CABLES / CORDS
VP-728900	Four-conductor cable #20. Alpha Wire Corp #2256-
4. SEE PCAS 1065 Color coded black, white, red, green.
VP-728950	Two-conductor annunciator cable. Otis Cable Spec
#2. BWI part #1262E002.
VP-729330	Two-conductor shielded cable, 20 gauge. Belden
part #8412.

	Page 10

Subject	VP#	Description
CABLES / CORDS
VP-729560	Six-conductor stranded cable, 20 gauge.
Manhattan part # M1006. 
VP-730550	Ten-conductor selector cable. Otis Cable Spec. #5.
VP-753365	Four-conductor type `SO' cable, 18 gauge.
VP-753430	Linen lacing cord. #9-6 holdfast waxed linen cord.
VP-753500	Two-conductor, type `SO' cable, 14 gauge.
VP-753550	Four-conductor, 12 AWG cable. Multi-conductor,
variable frequency drive cable for use on 5 to 15 hp motors.
VP-753555	Four-conductor, 8 AWG cable. Multi-conductor,
variable frequency drive cable for use on 20 to 25 hp motors.
VP-753560	Four-conductor, 6 AWG cable. Multi-conductor,
variable frequency drive cable for use on 40 to 50 hp GEM motors.
VP-753565	Four-conductor, 4 AWG cable. Multi-conductor,
variable frequency drive cable for use on 50 hp, 900 rpm GEM motors.
VP-753570	Four-conductor, 10 AWG cable. Multi-conductor,
variable frequency drive cable.
VP-753650	Two-conductor, type `S' cable. 16 gauge.
VP-753850	Two-conductor, type `SJ' cable, 18 gauge.
VP-753856	Four-conductor, type `SJO' cable, 18 gauge. SEE C‑
3055, PCAS 1065
VP-753950	Two-conductor, type `SO' cable, 18 gauge.
VP-754150	Four-conductor, shielded communication cable, 20
gauge. Belden part #8424.
VP-754155	Electrical cable, 22 gauge, 4 conductor, twisted.
VP-901700	Twine, #36 cable cord, 1/2-lb. balls.
VP-917500	Communication cable, 2/C, 22 AWG (7/32) TC, 500
ft. reel, (.81 mm) PVC jacket, 75 C type CM or AWM use: internal/external interconnection of elec.equip.

	Page 11

Subject	VP#	Description
CAPS, BRUSH
CAPS, BRUSH
VP-723468	Brush cap for 6333CG1 & 6333CG2 door motors.
Indiana General Motor Prod. # BHC-249.
VP-732311	Orange brush holder protective cap. Caplug #7/8,
SC-7/8. 
CHAINS
VP-735210	USE P/N: AAA332BP1. 1/4" brass oil chain. For
motor bearing sleeves & secondary sheave bearing sleeves.
VP-735850	Elwell twist chain; machine chain-twist link; trade
size #4. 
VP-736100	#6 steel cable chain. Rexnord Inc. #6H5.
VP-736150	2 x 2 leaf chain, 3/8" pitch. Chain Engineering part
# AL-322.
VP-736300	#35 chain, 3/8" pitch, rollerless.
VP-736450	#40 2x2 steel cable chain, 1/2" pitch, 5.5 feet long.
Used on Otis 6146B cam operating device.
VP-736500	#40 roller chain.
VP-736700	#41 roller chain, 1/4" wide, 1/2" pitch. Used on
6806A vertical lifting car gate; 40A, 42A, 43A door closers; vertical bi-parting doors.
VP-736975	#148 diamond chain, 1/4" wide, 5/8" pitch.
CLAMPS / CLIPS
VP-737850	Spring Clamp, 1-inch max opening, constructed of
high-tech resin material making clamp strong, lightweight and rust resistant. Clamp features soft, durable pads to protect fine finishes.
VP-738325	1-1/4" muffler clamp. 
VP-741175	C-10 pull strap clip. 16-gauge galvanized steel.
VP-741965	Splice clips for damaged selector tape. 
VP-741980	Mueller Electric #45 clip with screws.
VP-804614	Beam clamp. Part of VP-804615, Top-of-Car Insp.
Light.

	Page 12

Subject	VP#	Description
CLEANERS
CLEANERS
VP-420400	Polish, Lemon trigger, 16 oz.
VP-420410	Stainless steel cleaner and polish. In 1 quart bottle
w/ pump nozzle. Water based, environmentally safe. 
VP-420420	Cleaner for plastic, glass and metal. In 16 oz. spray
can, Non-ozone depleting. Used for e*Display.
VP-420422	Presaturated alcohol wipe. 6in x 6in packed
individually. 50 per carton. For final cleaning of small surface areas before applying adhesives or coatings.
VP-420478	Cleaner # 10, in 12 ounce net wt. aerosol can.
Replaces cleaner #9. 
VP-420481	Crystal Simple Green. Premixed 3-1/2:1 in 1 gallon
containers. 
VP-420482	Crystal Simple Green. Premixed 3-1/2:1 in 55
gallon drum. 
VP-420535	Cleaning Compound #2 in 1 quart containers. 
VP-420540	Cleaning Compound #2 in 1-gallon containers. 
VP-420545	Cleaning Compound #2 in 5-gallon drums. 
VP-420550	Belt Treatment-GBW in 1 quart containers. Special
treatment for Gen2 belts. Replaces temporary part number VP-420535-GBW. 
VP-740001	Dust mop treatment solution, water-based. In 1
quart bottle.
VP-740549	Towlette type hand cleaner, pre-moistened.
"Waterless Hand Wipes" Used to remove grease, adhesives, ink, lubricants, and more.
VP-740550	Hand cleaner with pumice. In 4.5 pound cartridge
for use in VP-740550, 6 per carton. Waterless, lemon scented. 
VP-740551	Dispenser for waterless hand cleaner, VP-740550.

	Page 13

Subject	VP#	Description
CLEANERS
VP-740552	Hand cleaner with pumice. In 18 ounce container,
12 per carton. Waterless, lemon scented. 
VP-765900	PC board edge cleaner. In 11oz. container.
12/case. Used in MRVF Maintenance Tool Kit, VP-798700.
CLIPBOARD
VP-741100	Saunders metal "snapack" clipboard with Otis
logo.
CLIPS
VP-738500	Binder clip. 1" capacity.
VP-738550	Glove clip. To clip and hold one pair of work
gloves. Used in VP-754201 and VP-754202 safety bags.
CLOTH
VP-702000	Abrasive pad, 6" x 9.5" - nylon cleaning pad,
green
VP-702001	Abrasive pad, Scotch Brite type, Light Duty: White
VP-702002	Abrasive pad, Scotch Brite type, Heavy Duty: Tan
COILS
VP-743790	Coil kit for BDC relay. Prestolite Electric part
number JBA-501FS.
VP-743813	EECO coil # S-752L, 110 volts DC.
CONNECTORS
VP-749810	Connector, Buchannan part # PCB3A-36A.
CONTACTS
VP-752300	Contact kit per M.L. 2185C2 with contact 153F1
for mounting on floor bar per drawing 7565D.
VP-752302	Contact kit per M.L. 2185C4 with contact 153E1
for mounting on floor bar per drawing 6575D.
VP-752303	Contact kit for BDC relay. Prestolite Electric part #
JAS-3001S.

	Page 14

Subject	VP#	Description
COUPLINGS
COUPLINGS
VP-755150	Flexible motor coupling, 5/8" x 3/4", for AC `O'
operators without brake, and DC `O' operators. Lovejoy Coupling # L 075.
VP-755800	Coupling for 7770R door motor encoder kit,
Renbrandt # C31F25R. USED IN KIT: VP-798605
VP-798540	Wood's Sure-Flex coupling. 
COVERS
VP-756450	Cover for emergency stop switch on J escalator.
DASHPOTS
VP-760800	Dashpot, Allen Bradley # X401-88-800-01. Dashpot
assembly without plunger or cap.
DECALS
VP-760820	Decal strips, "480 VOLTS". Four decals per strip.
Brady part #44215.
VP-760850	Decal, "PLEASE HOLD HANDRAIL". Red lettering on
white background.
DEVICES
VP-761040	9" monomass device.
VP-877600	SEE STAPLE REMOVER.
DOOR LOCKS
VP-843580	Hoistway door lock/roller device.

	Page 15

Subject	VP#	Description
DOOR SILENCERS
DOOR SILENCERS
VP-461480	Rubber door silencer. McMaster Carr #1432A11.
DRILLS
VP-762300	Fractional twist drills in waterproof case, sizes
1/16 through 1/2 inch (by 1/64)
VP-762410	3/16" Carbide-Tipped Masonary Drill Bit, 3" long
with a 3/16" Shank.
VP-762500	1/4" masonry drill, 4" regular spiral.
VP-762550	1/2" high helix masonry drill, 6" long, with 3/8"
shank.
VP-762726	Drill bit 'F' size. For use with assembly
CAA24350C1, 7300 D.C. operator conversion assembly.
VP-762800	`Q' size drill bit, standard length. 
VP-763200	Drill bit #7, standard length.
VP-763400	Drill bit #11, standard length.
VP-763700	Drill bit #21, standard length.
VP-763750	Drill bit # 25, standard length.
VP-763950	Drill bit #29, standard length.
VP-764152	#47 drill bit.
VP-764350	1/16" drill bit, standard length.
VP-764400	5/64" drill bit, standard length.
VP-764450	3/32" drill bit, standard length.
VP-764500	7/64" drill bit, standard length.
VP-764550	1/8" drill bit, standard length.
VP-764600	9/64" drill bit, standard length.
VP-764650	5/32" drill bit, standard length.
VP-764700	11/64" drill bit, standard length.
VP-764750	3/16" drill bit, standard length.
VP-764800	13/64" drill bit, standard length.
VP-764850	7/32" drill bit, standard length.
VP-764859	Drill Bit #1 (.228), standard length.
VP-764860	Drill Bit # 2 (.221), standard length.

	Page 16

Subject	VP#	Description
DRILLS
VP-765000	1/4" drill bit, standard length.
VP-765025	1/4" drill bit, high speed steel, extended reach. 12"
long.
VP-765100	17/64" drill bit, standard length.
VP-765150	9/32" drill bit, standard length.
VP-765250	5/16" drill bit, standard length.
VP-765300	21/64" drill bit, standard length.
VP-765350	11/32" drill bit, standard length.
VP-765450	3/8" drill bit, standard length.
VP-765500	25/64" drill bit, standard length.
VP-765550	13/32" drill bit, standard length.
VP-765600	27/64" drill bit, standard length.
VP-765602	27/64” drill bit, short length. 27/64” drill bit has a
2” flute with an overall length of 3-3/8”.
VP-765650	7/16" drill bit, standard length.
VP-765800	1/2" drill bit, standard length.
VP-765802	1/2” drill bit, short length. 1/2” drill bit has a 2-1/4”
flute with an overall length of 3-3/4”.
VP-765805	17/32" drill bit, high speed steel, standard length.
VP-765818	11/16" drill bit, high speed steel, standard length. 
VP-765830	Solid type drill guide, 15/32" O.D. x 1-3/16" long.
For 3/16" drill. Snap-On P/N E1521. Application: 17CT gear installation, 
VP-765840	Step drill bit; 1/8" to 1/2" in 1/32" increments; 13
hole sizes; 1/4" shank; 1/8" step thickness; self-starting tip. Was P/N REP-UNIBIT1
VP-765841	STEP drill bit; 3/16" to 1/2" in 1/16" increments; 6
hole sizes; 1/4" shank; 3/8" step thickness; self-starting tip. WAS P/N REP-UNIBIT5
VP-765842	Step drill bit; 3/16 to 7/8"in 1/16" increments; 12
hole sizes; 3/8" shank; 1/8"step thickness; self-starting tip. Was P/N REP-UNIBIT14
VP-765843	Step drill bit; 1/4" to 3/4" in 1/16" increments; 9
hole sizes; 3/8" shank; 1/8" step thickness; self-starting tip. Was P/N REP-UNIBIT3.
VP-770050	Carbide bur, A-41D 3/32 x 3/8 x 1-1/4.

	Page 17

Subject	VP#	Description
FILES
FILES
VP-770160                                      8" half round mill bastard file.
VP-770200	10" half round mill bastard file.
VP-770250	12" half round mill bastard file.
VP-770300	14" half round mill bastard file.
VP-770400	6" mill bastard file.
VP-770450	8" mill bastard file.
VP-770500	10" mill bastard file.
VP-770550	12" mill bastard file.
VP-770750	File Board Industrial Supplies Co.
VP-770800	6" round mill bastard file.
VP-770950	12" round mill bastard file.
VP-771850	6" half round bastard file.
VP-772350	14" flexible vixon rail file.
VP-772700	8" round machinist file, 2nd cut.
VP-772750	8" taper file.
FILTERS
VP-772930	Door operator filter. Consists of: one A234E1
choke; one P303CG8 terminal block; and two P226FC1 capacitors.
VP-772951	Filter, Glassfloss hi-pack material, 8-3/4" x 8-3/4"
x 1/2" Vendor P/N 8-3/4x8-3/4x1/2
FIRST AID
VP-773000	First aid kit, Swift 34-600H One-person kit.
VP-773001	First aid kit, Swift 34-0025. 25-person kit.
VP-773002	Non-aspirin pain reliever. 250 packs per box, 2
tables per pack. One box equals one piece.
VP-773003	3/4" x 3" plastic bandaids, in box of 100.
VP-846400	First Aid Kit, 50 person

	Page 18

Subject	VP#	Description
FLAGS
FLAGS
VP-774900	Safety flag for pole barricades outlined in Circular
Letter 2565 in `G' Manual.
FLASHLIGHT
VP-800205-2	Streamlight ENDURO® LED 2AAA Headlamp. .5
watt, 100,000 hour life, Up to 6 hrs, runtime on high; up to 24 hrs on low. Impact-resistant, Waterproof, 2.75oz w/battery and head strap. (batteries included).
VP-800206	Replacement Bulb for Headlamp, VP-800205.
Package of 2 bulbs. Drop Ship item.
VP-800216	PolyStinger w/out Charger - Yellow - This is the
Poly-Stinger Flashlight & battery stick only. It does not come with any chargers/holders. You would only buy this if you already have your charger/holder.
VP-800217	Polystinger Yellow with AC/DC fast piggyback
charger - Comes complete with both AC (home) cord, DC 12-volt (car lighter) cord & a FAST (2.5 hour) piggyback charger/holder with spare battery.
VP-800218	Polystinger Yellow with DC fast piggyback charger - This YELLOW Poly-Stinger Rechargeable flashlight system comes with 12-volt DC (car) cord, 1 FAST (2.5 hour) Piggyback charger and 1 extra battery
VP-800219	Stinger Battery Stick - Replacement battery stick
for the Streamlight Stinger, Stinger HP, Stinger XT, Stinger XT HP, PolyStinger.
VP-800220	Stinger Bulb (Stinger, Stinger XT, PolyStinger)
VP-800221	Stinger Piggyback charger holder. Includes an extra
battery for your stinger flashlight and will charge a flashlight and extra battery at the same time. AC 120v & DC 12v cords sold separately.
VP-800222	This 120 volt AC (home)Charge Cord fits all
Streamlight rechargeable cradles, holders & sleeves.
VP-800223	This 12 volt DC (car)Charge Cord fits all Streamlight
rechargeable cradles, holders & sleeves

	Page 19

Subject	VP#	Description
FUSEHOLDER
FUSEHOLDERS
VP-779790	Fuseholder, Bussman.
FUSES
VP-775000	Kit of 115 glass fuses in plastic case. Within case
fuses come in packs of five. Fuses range in size from 1/8 Amp to 10 Amps. Types ABC, AGC, & MDL (glass) 250V, 1-1/4" long.
VP-776500	Fuse, AGC 6-1/4 amp.
VP-776600	Fuse, Bussman # AGX, 8 amp.
VP-778400	Fuse, Littlefuse #512001, normal-blo, 1 amp.
VP-778410	Fuse, Littlefuse #523003, slo-blo, 3 amp.
VP-778420	Fuse, Littlefuse #523005, slo-blo, 5 amp.
VP-778500	Fuse, Littlefuse, #3AG, slo-blo, 1/4 amp. Lower
level component of Lambda detector assembly, Otis part #1F-6971AF1.
GAL
VP-782005	T' power pack for GAL light ray. 
VP-782019	Keyswitch marked "INSPECTION" with GAL type
HA1612 key. 
VP-782020	Keyswitch marked "OFF-ON-FIRE SERVICE" with
GAL type FSS1617 key. 
VP-782021	Keyswitch marked "LIGHT-FAN" with GAL type STD1601 key, 3-position. 
VP-782023	Keeper release assembly, GAL # MO-IO Keeper
Release Assy., RH. 
VP-782024	Keeper release mounting plate; GAL # MO-IO
Keeper Release Mounting Plate Only w/Roller, RH.
VP-782025	Keeper release assembly w/mounting plate; GAL #
MO-IO Kpr. Rel. Assy. w/Mounting Plate. 
VP-782027	GAL hall button; GAL type RRB hall button for Otis
LRV program.

	Page 20

Subject	VP#	Description
GAL
VP-782033	Key for GAL type HA1612 keyswitch used on Otis
program. 
VP-782034	Key for GAL type 1613 keyswitch used on Otis LRV
program. 
VP-782035	Key for GAL type FSS1617 keyswitch used on Otis
LRV program. 
VP-782036	Key for GAL type STD1601 keyswitch used on Otis
LRV program. 
VP-782038-1	Floor button assy. GAL type RRB button marked `1'
for Otis LRV program; uses 120V bulb. 
VP-782038-2	Floor button assy. GAL type RRB button marked `2'
for Otis LRV program; uses 120V bulb. 
VP-782038-3	Floor button assy. GAL type RRB button marked `3'
for Otis LRV program; uses 120V bulb. 
VP-782038-4	Floor button assy. GAL type RRB button marked `4'
for Otis LRV program; uses 120V bulb. 
VP-782038-DOOR CLOSE	Button assembly. GAL type RRB button marked
"DOOR CLOSE" for Otis LRV program. 
VP-782038-DOOR OPEN	Button assembly. GAL type RRB button marked
"DOOR OPEN" for Otis LRV program. 
VP-782040	Switch. GAL car operating panel Emergency Stop
switch for Otis LRV progam. 
VP-782200	Nylon pivot pin, for MODP GAL campack cams.
1/8" diam x 5/8" long. For units mftd prior to 11/1970
VP-782201	Nylon pivot pin, for MODP GAL campack cams.
5/32" diam x 5/8" long. For units mftd after 11/1970

	Page 21

Subject	VP#	Description
GASKETS
GASKETS
 VP-782950	Gasket, Winsmith part #2620. 
GAUGES
VP-769150	Feeler gauge stick, .03". Starrett #667-30. Used in
MRVF Maintenance Tool Kit, VP-789700.
GIBS / GUIDES
VP-784500	EPCO H-D3 door gib assembly. Includes 1" wide,
`D3' chassis with 17/32" wide, green `H' gib and hardware.
VP-785000	EPCO CG-D4 door gib assembly. Includes 1-1/8"
wide, `D4' chassis with 15/32" wide, black `CG' gib and hardware.
VP-785100	EPCO `R' rail guide shoe gib, nylon.
VP-785150	EPCO `RH' rail guide shoe gib, nylon.
VP-785200	EPCO `W' rail guide shoe gib, nylon.
VP-789400	EPCO T-D3 door gib assembly. Includes 1" wide,
`D3' chassis with 1/2" wide, blue 'T' gib and hardware.
VP-789450	EPCO T-D5 door gib assembly. Includes 1-1/4"
wide, `D5' chassis with 1/2" wide, blue 'T' gib and hardware.
VP-790153	EPCO C-D3 door gib assembly. Includes 1" wide,
`D3' chassis with 15/32" wide, white 'C' gib and hardware.
VP-790154	EPCO CD-4 door gib assembly. Includes 1-1/8"
wide - 10 gib adjustments "D-4" chassis with 15/32" wide, white "C" gib and hardware.

	Page 22

Subject	VP#	Description
GLOVES
GLOVES
VP-846101	Dyneema stretch fit glove with rubber coating. Size
XXS. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 Pair
VP-846102	Dyneema stretch fit glove with rubber coating. Size
XS. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 pair
VP-846103	Dyneema stretch fit glove with rubber coating. Size
S. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846104	Dyneema stretch fit glove with rubber coating. Size
M. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846105	Dyneema stretch fit glove with rubber coating. Size
8.5. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846106	Dyneema stretch fit glove with rubber coating. Size
L. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846107	Dyneema stretch fit glove with rubber coating. Size
XL. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846108	Dyneema stretch fit glove with rubber coating. Size
XXL. Cut resistant with increased dexterity. Coated palm and fingers for gripping any surface. 1 PAIR
VP-846109	Dyneema stretch fit glove with rubber coating. Size
XXXL. Cut resistant with increased dexterity.
Coated palm and fingers for gripping any surface. 1 PAIR
VP-846225	Gloves, Nitrile dipped Predator work gloves. 1
dozen pair. Size: Large.
VP-846230	Heavy duty leather palm work glove. Size jumbo. 1
pair. With seamless kevlar lining providing cut and slash protection, green cuff. Drop Ship item.
VP-846231	Heavy duty leather palm work glove. Size men. 1
pair. With seamless kevlar lining providing cut and slash protection, red cuff. Drop Ship item.

	Page 23

Subject	VP#	Description
GLOVES
VP-846233-1-10	Leather work gloves, size 10. For use with Arc Flash
PPE.
vp-846233-1-11	Leather work gloves, size 11. For use with Arc Flash
PPE.
VP-846233-1-9	Leather work gloves, size 9. For use with Arc Flash
PPE.
VP-846235	Kevlar seamless knit glove with sewn in leather
palm. Size jumbo. 1 pair. Heat, cut and slash resistant, blue cuff. Drop Ship item.
VP-846236	Kevlar seamless knit glove with sewn in leather
palm. Size men. 1 pair. Heat, cut and slash resistant, brown cuff. Drop Ship item.
VP-846237	Kevlar seamless knit glove with sewn in leather
palm. Size ladies. 1 pair. Heat, cut and slash resistant, red cuff. Drop Ship item.
VP-846257-1-10	Rubber Insulating Gloves, 11" class 00, size 10.
ASTM D120.
VP-846257-1-11	Rubber Insulating Gloves, 11" class 00, size 11.
ASTM D120.
VP-846257-1-9	Rubber Insulating Gloves, 11" class 00, size 9.
ASTM D120.
VP-846257-2-11	Leather Protectors, BSL GPL V, size 11. For use
with VP-846257-1-11.
VP-846257-2-9	Leather Protectors, BSL GPL V, size 9. For use with
VP-846257-1-9.
VP-846260	High durability, heat resistant mechanics gloves
with double layered palm. Three fingertips cut out for increased dexterity. Washable. Size small. 1 pair. Drop Ship item.
VP-846261	High durability, heat resistant mechanics gloves
with double layered palm. Three fingertips cut out for increased dexterity. Washable. Size medium. 1 pair. Drop Ship item.
VP-846262	High durability, heat resistant mechanics gloves
with double layered palm. Three fingertips cut out for increased dexterity. Washable. Size large. 1 pair. Drop Ship item.

	Page 24

Subject	VP#	Description
GLOVES
VP-846263	High durability, heat resistant mechanics gloves
with double layered palm. Three fingertips cut out for increased dexterity. Washable. Size X-large. 1 pair. Drop Ship item.
VP-846264	High durability, heat resistant mechanics gloves with double layered palm. Three fingertips cut out for increased dexterity. Washable. Size XX-large. 1 pair. Drop Ship item. 
VP-846270	High durability, heat resistant mechanics gloves
with double layered palm. Full fingertips. Washable. Size small. 1 pair. Drop Ship item.
VP-846271	High durability, heat resistant mechanics gloves
with double layered palm. Full fingertips.
Washable. Size medium. 1 pair. Drop Ship item.
VP-846273	High durability, heat resistant mechanics gloves
with double layered palm. Full fingertips.
Washable. Size X-large. 1 pair. Drop Ship item.
VP-846274	High durability, heat resistant mechanics gloves
with double layered palm. Full fingertips.
Washable. Size XX-large. 1 pair. Drop Ship item.
VP-846391	Gloves, nitrile (size 10), 15 mil, solvent-resistant.
One Pair. 
VP-846392	Gloves, welding, box of 12
VP-846393	Gloves, work with leather palm, box of 12
VP-846394	Latex gloves, disposable, 50 pair per dispenser,
non-sterile, ambidextrous, size medium.
VP-846395	Latex gloves, disposable, 50 pair per dispenser,
non-sterile, ambidextrous, size large.
VP-846396	Latex gloves, disposable, 50 pair per dispenser,
non-sterile, ambidextrous, size X-large.
GRILLS
VP-788100	Plastic grill for E311/411M controller door. Rittal
#3161.
GROMMETS
VP-788275	Rubber grommet, 1-1/4". 

	Page 25

Subject	VP#	Description
GUARDS
GUARDS
VP-788480	Traveling cable scuff guard.
VP-911701	Triangle Corner Protector. Yellow Triangle, Size -
.062. For 16 GA. Material.
HEATERS
VP-792553	Heater, plug type, fits 1/4" pipe plug hold, 25W,
110V, for use in door operators. Hotwatt
#13E0031-1. Use with VP-896660 thermostat.
HINGES
VP-792810	Hinge, SOSS type 314 with dull brass finish.
HOSES
VP-793900	Hose, 3/4" inside diameter, 3-braid Goodyear
ortac red neoprene.
INK
VP-708651	Dykem Steel Blue Layout Fluid. 8 oz. bottle with
applicator brush in cap.
INSULATORS
VP-795080	Red insulator, Mueller Electric #47. Used to
assemble VP-796075 jumper clips.
JEWELS
VP-796000	SEE ADHESIVES / SEALANTS.
KEYS
VP-796300	Key, Eagle #A36A4, for car operating panels and
telephone cabinets.
VP-796345	Key for Otis type 431Y lock. Corbin key # BGM30
used with lock #219K09-5.
VP-796350	Key for Otis type 6410R switch assy. Used for light
switches and independent service in COP. Arrow Hart #1561-488.
VP-796400	Gamma 'D' cabinet key
VP-796595	Key for over-the-door lockboxes. For use with VP‑
811720, VP-811725 and VP-811730 lockboxes. 

	Page 26

Subject	VP#	Description
KEYS
VP-796810	Key Eagle # A36A123 used for car operating panels
and telephone cabinets.
VP-796840	Key, Corbin #4T74635. For lock P/N 431T1
VP-796850	Key, Yale & Towne #47, for starter panels.
VP-796905	Key # GA27248 for Otis lock #s 431C3, 431C6, and
179379.
VP-797050	Key, Yale & Towne #14398GB, primarily for car top
access.
VP-797100	Key, Yale & Towne #18549E, primarily used for
generator starting switches on older units.
VP-797110	Key, Yale & Towne #5957 for Otis type 6410T
keyswitch. Chicago & ANSI SES
VP-797120	Key, Yale #2642 for New York SES.
VP-797130	Key, Yale #3502. Used on AAA7069BH keyswitch
assemblies. Mass. SES
VP-797135	Key, Yale #1254. Used on AAA431AM1 5-pin cab
top exit lock.
VP-797140	Key, Chicago #BFD1 for Ace type lock. Used for
AAA7069BH keyswitch assemblies.
VP-810385	Key, Chicago #7306. Used with VP-810380.
KITS
VP-700800	SEE ANTI-STATIC.
VP-700801	SEE ANTI-STATIC.
VP-752300	SEE CONTACTS.
VP-766100	Kit for inserting and extracting eproms. 5 pieces.
For eproms with 14 - 40 pins. Vendor: Contact East. P/N: WK-7.
VP-773000	SEE FIRST AID.
VP-773001	SEE FIRST AID.
VP-775000	SEE FUSES.
VP-789700	SEE MRVF.
VP-798000	Kit OF 3/4" pipe fittings for 17CT gear box
standpipe kit. 

	Page 27

Subject	VP#	Description
KITS
VP-798420	USE P/N: AAA6942FT5. Gorman kit for converting
single packing 5" welded head to double packing, HVP/HVH only, w/out 386BGD3. 
VP-798460	Piping kit for hydraulic elevators; pressure switch
to comply with ANSI & CSA Safety Codes.
VP-804608	Kit, Hardware for top-of-car inspection light, VP‑
804615.
LABELS
VP-420486	Hazard Information label for Crystal Simple Green
cleaner. To be used on any secondary container of Simple Green.
VP-865050	MSDS access information card. Includes toll free
telephone numbers and other contact information for 3E Company. Also includes list of information to have available when requesting an MSDS.
LAMPS
VP-800475	Lamp, Dialco #507.
VP-800650	Bayonet base miniature lamp, GE #88, S-8, 15W,
1.91 amp. 
VP-800670	Lamp, GE #238. 
VP-800700	Bayonet base miniature lamp, double contact.
Sylvania #1004.
VP-800800	Indicator lamp, miniature screw base. Sylvania
#1487, T 3-1/4, 14V, .20 amp.
VP-800850	Lamp, GE #1476.
VP-800900	Lamp, Sylvania #1477, 24V.
VP-801740	Lamp, subminiature. T-1-3/4 type bulb, wedge
type base. 5 Volt, 0.115 Amp. 0.8" tall.
VP-801750	Clear lamp, 6S6, 6W, 155V.
VP-802625	Lamp, 30V, 6W, Screw type base. Drop Ship Item.
VP-803860	Lamp, Sylvania #381, T 1-3/4, 6.3V, .55C.

	Page 28

Subject	VP#	Description
LIGHT FIXTURES
LIGHT FIXTURES
VP-804550	Comblite, 3" diameter, bronze. Complete assembly
of lens & frame.
VP-804555	Comblite, 3" diameter, stainless steel. Complete
assembly of lens & frame.
VP-804600-2	Ericson Pivot Light. Base magnet, NEMA 5-15
power outlet in handle, 13 watt fluorescent bulb provides same light output as 60 watt incandescent without the intense heat, Scratch and shatter resistant lens, Oil and water resistant power cord, Yellow.
VP-804616	20-foot drop light, 100 watt incandescent. Without
outlet, with switch. Plastic body and cage.
VP-810221	Nylube surface mounted emergency light fixture,
stainless steel finish; with 6V battery and 120VAC wiring terminals.
VP-810222	Nylube surface mounted emergency light fixture
for mounting above translucent ceiling; with 6V battery and 120VAC wiring terminals.
VP-810224	Nylube CSA approved car-top power supply w/
remote, surface mounted, slimline emergency light fixture; with 6V battery and 120VAC wiring terminals.
VP-810225	EPCO surface mounted emergency light fixture,
bronze finish. 
LOCKBOX
VP-811720	Lockbox, over-the-door, without key. Use key VP‑
796595. 
VP-811725	Lockbox, knob type, without key. Use key VP‑
796595.
VP-811730	Lockbox, credit card style, over-the-door type,
without key. Can hold a credit card, or
approximately 10 keys. Use key VP-796595.

	Page 29

Subject	VP#	Description
LOCKS
LOCKS
VP-729013	Master super security hasp 6X700, and decal with
the following text: "PROPERTY OF OTIS ELEVATOR CO."
VP-810380	Lock, Chicago Lock #41531W90 with circular key
#7306, one-way, 90 degrees.
VP-810400	Combination padlock, 5/16" O.D. Hardened Hasp
VP-810410	Keyed padlock for Lockout/Tagout. 1/4" hasp.
Includes identification labels.
VP-810415	Two keyed padlocks matched to same key (4
identical keys included). For Lockout/Tagout. 1/4" hasp. Includes identification labels.
LUBRICANTS
VP-418785	Oil #2 in 1 quart containers. Used for sleeve type
bearings on motor generators, etc. 
VP-418790	Oil #2 in 1 gallon cans. Used for sleeve type
bearings on motor generators, lubrication of escalator chains, etc. 
VP-418935	Oil #10 in 1 gallon cans. 
VP-418940	Oil #10 in 5 gallon cans 
VP-418990	Oil #16 in 1 gallon can. Otis water hydraulic lube.
Emulsifying oil for use in water hydraulic elevators. 
VP-419150	Oil #47 in 1 quart pour spout bottles. Replaces Oil
#26, VP-419140. Replaces Oil #5, VP-418890. 
VP-419240	Oil #31(previously #31A) in 1 gallon cans. Guide
rail lube. 
VP-419241	Oil #31(previously #31A) in 1 quart containers.
Guide rail lube. 
VP-419330	Oil #33 in 1 gallon cans. Worm gear oil.	
VP-419390	Oil #33 in 5 gallon cans. Worm gear oil.	
VP-419400	Oil #LO33A & #46. In 5 gallon can. Synthetic oil for
escalator machines.
VP-419540	Oil #35 in 10 ounce resealable plastic bottle. Dow
Corning silicone fluid type 200 (100 centistokes). For relay dashpots-silicone base. 

	Page 30

Subject	VP#	Description
LUBRICANTS
VP-419590	Oil #38 in 1 gallon cans for gearless machines and
secondary sheave bearings. 
VP-419690	Oil #39, In 1 gallon container. Escalator chain
lubricant. 
VP-419745	Oil #45, synthetic gear oil 460, in 5 gallon can. 
VP-419747	Oil #45, synthetic gear oil 460. In 1 gallon
container. 
VP-419748	Grease #17 in 14 oz. (400g.) grease gun tubes.
Synthetic grease compatible with Otis Oil #45 and #46. Must be used in bearings of gearboxes using oil #45.
VP-419750	Oil #60 in 1 gallon cans. Wire Rope Lubricant. 
VP-419755	Oil #60 in 1 quart containers w/pour spout. Wire
rope lubricant. 
VP-419760	Oil #60A, (synthetic). In 1 gal container. Synthetic
wire rope lubricant for use on Elevators and shuttle installations. 
VP-419775	Oil #41 in plastic one quart bottles with pour
spouts. Door operator oil. 
VP-419780	Synthetic oil in 1 quart bottles of 5W-30 Mobil 1
for cold weather use in door operators and checks. 
VP-419800	Air compressor oil, Mobil Rarus 427 in 1 quart
bottles. For use on MT-113001 and other single and multi-stage reciprocating air compressors. 
VP-419805	Oil #42 in 5 gallon cans. Hydraulic buffer Oil. Refer
to SS-22-76 for usage. 
VP-419806	Oil #42 in 1 gallon cans. Hydraulic buffer Oil. Refer
to SS-22-76 for usage. 
VP-419820	Oil #43 in 1 gallon plastic jugs. Helical gear Oil
VP-419830	Oil #59 in 1 gal. Containers. Used for maintenance
of non-Otis equipment. Helical Gear Oil, ISO 320. 
VP-419835	Oil #59 in 5 gal. Containers. Used for maintenance
of non-Otis equipment. Helical Gear Oil, ISO 320. 

	Page 31

Subject	VP#	Description
LUBRICANTS
VP-420040	Grease #14 in 10 ounce squeeze tube. Open gear
lubricating grease for external gears of machines and selector bevel gears. 
VP-420240	Grease #12 in 14 oz. grease gun tubes. For use on
ball/roller bearings & general greasing. 
VP-420243	Grease # 15, lithium, in 8 ounce squeeze tube.
Used for lubricating brake cores, bushings & sliding parts. 
VP-420245	Grease #12 in 5 gallon cans. For use on ball & roller
bearings & for general greasing. 
VP-420255	Otis Grease # 16 in 400 gram (14 oz) grease gun
cartridge. Special grease, first used for NCT travolator lubrication and certain bearings subject to low frequency oscillation or vibratory motion. 
VP-740553	Spray lubricant, LPS2 in 11oz. Aerosal spray bottle. Replaces WD-40 type lubricant. 
VP-740557	Derma shield hand protector in 6 oz. can. Sold by
case. 12, 6 oz. cans per case. 
VP-740565	#207 Fluid Film® NAS in 12oz. Non-aerosol pump
spray can (refillable). Rust and corrosion preventative and lubricant. 
VP-740566	#207 Fluid Film®, In 1 gallon refill can.
Rust/corrosion preventative and lubricant. 
VP-740575	Hole tapping lubricant, Tapfree 2, in 4 ounce
bottles. Good for Low and Med. Carbon steels, Cast Iron, Mild Stainless Steel, and Alloy Steels. Minimum order of 6. 
VP-740600	Copper Based Anti-seize lubricant,Loctite 51001
C5-A® in 1 oz. tube. Protects metal parts from rust, corrosion, galling and seizing at temps to 1800 deg. F. 
VP-740650	Gasket lubricant: Victaulic Lubricant, 4.5 oz. Tube.
To lubricate Victaulic fittings. 
VP-747000	Anti-Oxidation compound, Noalox® in 4 ounce
tube. Used in MRVF retrofit kit: Battery
Temperature Sensor. Improves surface life of aluminum electrical applications.

	Page 32

Subject	VP#	Description
LUBRICANTS
VP-794060	Silicone lubricant, LPS Heavy Duty Silicone, in 13 oz
aerosol can. Colorless and Odorless, eliminates squeaks, binds and sticking. 
VP-820410	Nyebar Type Q, 0.2% solution in two-oz. bottle;
stops oil creepage on motor & generator shafts. Replaces Type K from 2002 on.
VP-821600	Oil #36, in 5 gallon cans. Oil for hydraulic
elevators. 
VP-821610	Oil #36, in 55 gallon drum. Oil for hydraulic
elevators. 
VP-821620	Hydraulic elevator oil additive,1 quart. Comes with
one label AAA102AJG1. Used to eliminate "stiction". 
VP-821625	Oil # 52, in 1 gal. Containers. Used for
maintenance of non-Otis equipment. Hydraulic Oil, ISO 68. 
VP-821630	Oil # 52, in 5 gal. Containers. Used for
maintenance of non-Otis equipment. Hydraulic Oil, ISO 68
VP-821640	Oil #51 in 5 Gal. Containers. Used for maintenance
of non-Otis equipment. Hydraulic Oil, ISO 46. 
VP-821650	Hydraulic oil (Tractor Hydraulic Fluid) in 5 gallon
containers. Used in Schindler inverted hydraulic elevators. 
VP-821655	Hydraulic oil (Tractor Hydraulic Fluid) in 55 gallon
containers. Used in Schindler inverted hydraulic elevators. 
VP-821670	ISO 320 R & O Oil in 1 quart container. For
maintenance of non-Otis equipment, including rail lubrication of Kone units with SGB type safeties. Rust and oxidation inhibited oil. 
VP-821680	Exxon Polyrex EP2 Grease in 14 oz. grease gun
tube. For maintenance of non-Otis equipment, including Hollister-Whitney geared machines. Special Polurea grease NGLI 2. 
VP-821685	Mobil SHC 636 in 5 gallon container. For
maintenance of non-Otis equipment, including Hollister-Whitney geared machines. PAO synthetic gear lubricant, ISO680. 

	Page 33

Subject	VP#	Description
LUBRICANTS
VP-822005	Oil #58 in 1 gal. Containers. Used for maintenance
of non-Otis equipment. Gear Oil. 
VP-822010	Synthetic Hydraulic Fluid, Mobil SHC 524 in 1
gallon containers. Used in Hollister Whitney Rope Gripper. 
VP-822100	Oil; silicone fluid, General Electric # SF-1154 in 2 oz. tubes. Used on Louis Allis drives. 
VP-871800	Slipit in 1 quart can. Replaces Nylube compound.
MANUALS
VP-812007	OTISCHEK User Guide. Contains OTISCHEK
instructions and software.
VP-812008	OTISCHEK Quick Guide. Contains Quick Guide and
Hall Call Version.
VP-812015	Elevonic Upgrade Installation manual
VP-812016	Elevator Management System Manual. Version
2.1.8 dated 1/2/97. Contains: Installation & Operation guide T.I.P. 27.5-9 with EMS wiring diagrams on drawings ABA7155BL, A7155AS.
VP-812033	Call Closeout Codes. For use with web-ready
phones. Publication date 9/5/2001.
VP-812256	Manual, bound, 8-1/2 x 11", EMS Panorama
Installation Guide.

	Page 34

Subject	VP#	Description
MARKERS
VP-811900	Marker, Permanent, black, sold individually
VP-811910	Red, fine point, paint pen. Water based, non-toxic
for marking of parts, components. Sold in package of 12.
VP-811911	White, fine point, paint pen for marking of parts,
components. Water based, non-toxic. Sold in package of 12.
VP-811912	"Real White", fine point, paint pen for touch-up.
Water based, non-toxic. Sold in package of 12 and in Owner Key Kits AAA23800D1 and 2.
MATS
VP-702100	Adhesive floor mats. 18" X 36" "Clean-Walk" mats.
Removes dirt and contaminants from shoe soles on contact. 30 sheets per mat.
VP-702101	Adhesive floor mats. 36" X 46" "Clean-Walk" mats.
Removes dirt and contaminants from shoe soles on contact. 30 sheets per mat.
VP-702105	Protective corrugated black vinyl mat. Conforms to
ASTM D178-93 Type I, Class 2. For use near controllers. 24" wide X 1/4" thick X 12 feet long.
MODULES
VP-812350	Module, Interface Products #2040.
MOPS
VP-740002	Mop - 3" Wide, 18" long mopheads with 54"
hardwood handle. 
VP-740003	Mop - 3" wide, 24" long mophead with 54"
hardwood handle
VP-740004	Mophead refill - 3" wide, for 18" long mophead
VP-740005	Mophead refill - 3" wide, for 24" long mophead

	Page 35

Subject	VP#	Description
MOTORS MOTORS
VP-708020	Cooling blower minus motor Dayton, P/N 1C792
Used with cooling blower kit: 2700ACB1
VP-708021	Cooling blower minus motor Dayton, P/N 1C791
Used with cooling blower kit: 2700ADD3
VP-814375	Motor, Morrison Products #06-0105-0; 1/20 H.P.;
for Otis part #6091T1 blower.
VP-814551	Motor, GE #5BCC56EB4B, 1/3 H.P., 115V DC; used
for `O' operator.
VP-814821	Motor, single phase, open drip-proof, 1/3 HP 1725
RPM, 115/208-230V , NEMA 48Y frame for cooling blower kit 2700ADD3
VP-814822	Motor, three-phase, open drip-proof, 1/3 HP, 1725
RPM, 208-230/460V, NEMA 48 frame for cooling blower kit 2700ACB1.
MRVF
VP-789700	MRVF Maintenance Tool Kit. Contains: MT‑
115030, MT-122014, MT-124027-1, VP-700300, VP-765900, VP-769150, VP-814900, VP-835100.
NUTS
VP-816540	Bearhug locknut #9 used in place of spanner nut &
lock washer. For locking bearings on to shafts. Whittet-Higgins # BH-09.
VP-816893	Nut, DIN 934 M8.
VP-816895	Nut, hex, DIN 934 M12
VP-816949	Steel locknut, DIN 985 M10 x 1.5, nylon insert.
VP-817250	Standard hex jam nut, 1/2", brass. Same as Otis
#69P5.
VP-817285	Standard hex nut, 5/8", steel.
VP-817340	Standard hex nut, 1/4", steel.
VP-817390	Hex machine screw nut, 10-32, brass. Double
chamfered, thread class 2B. Same as Otis #74E3.
VP-817400	Hex machine screw nut, 5-40, cadmium plated.
Double chamfered, thread class 2B. Same as Otis #74E2.

	Page 36

Subject	VP#	Description
NUTS
VP-818150	Hex nut, 3/4"-10, Zinc plated steel Grade 5. Used
in MT-102050 pipe stands.
VP-818410	Twirl nut.
VP-818420	Hex machine screw nut, 3/8", brass.
VP-818435	American Standard hex machine screw nut, 8-32,
brass. 11/32" across face x 1/8" thick, double chamfer.
VP-818510	American Standard CPR hex nut, 8-32, steel, coarse
thread, class two.
VP-818600	American Standard hex light jam nut, 3/8", steel,
fine thread, class two. Same as Otis #85D3.
VP-818725	Hex pal nut, 8-32, steel.
VP-819800	Hex nut, 10-32, steel, cadmium plated.
OIL CANS
VP-820100	8 oz plastic oil can with 5 inch flexible metal nozzle
and hand grip pump.
VP-829130	Pail, 6 gallon galvanized with cover.
PADS
VP-740100	Liquid absorbent pads. 16.5" X 20" mats.	50
	pads / bag.
VP-740101	Liquid absorbent rolled mat pads. 3 rolls / bag,
	each 4" wide X 150' long.
VP-740102	Liquid absorbent pads. Absorbs most liquids; oils,
coolants, solvents and water. 16.5" X 20" mats. 125 pads / bag.
VP-740103	Oil absorbent pads. Absorbs petroleum-based
liquids, but not water. 16.5" X 20" mats. 100 pads / bag.

	Page 37

Subject	VP#	Description
PAINTS
PAINTS
VP-829001	Zinc. Rust-oleum 20 ounce aerosol spray paint.
VP-829002	Rust Doctor, water based rust converter for steel
surfaces. Converts rust into a protective coating that inhibits further rusting. Also acts as a primer. 1 quart. Drop Ship item.
VP-830175	SEE PANS.
VP-902705	Capri Blue. Sherwin Williams Polyurethane Enamel.
11 ounce spray can. Drop Ship item.
VP-902706	Capri Blue. Sherwin Williams Polyurethane Enamel.
1 quart container. Drop Ship item.
VP-902707	Capri Blue. Sherwin Williams Polyurethane Enamel.
1 gallon container. Drop Ship item.
VP-902710	Aluminum. Sherwin Williams Enamel. 11 ounce
spray can. Drop Ship item.
VP-902712	Aluminum. Sherwin Williams Enamel. 1 gallon
container. Drop Ship item.
VP-902721	Beige / Flax. Sherwin Williams Polyurethane
Enamel. 1 quart container. Drop Ship item.
VP-902722	Beige / Flax. Sherwin Williams Polyurethane
Enamel. 1 gallon container. Drop Ship item.
VP-902730	Yellow. Sherwin Williams Polyurethane Enamel. 11
ounce spray can. Drop Ship item.
VP-902731	Yellow. Sherwin Williams Polyurethane Enamel. 1
quart container. Drop Ship item.
VP-902732	Yellow. Sherwin Williams Polyurethane Enamel. 1
gallon container. Drop Ship item.
VP-902740	Clear. Sherwin Williams Polyurethane. 11 ounce
spray can. Drop Ship item.
VP-902741	Clear. Sherwin Williams Polyurethane. 1 quart
container. Drop Ship item.
VP-902751	Paint odor eliminator. 8 ounce can.
VP-902760	Black. Sherwin Williams Polyurethane Enamel. 11
ounce spray can. Drop Ship item.
VP-902761	Black. Sherwin Williams Polyurethane Enamel. 1
quart container. Drop Ship item.

	Page 38

Subject	VP#	Description
PAINTS
VP-902762	Black. Sherwin Williams Polyurethane Enamel. 1
gallon container. Drop Ship item.
VP-902770	Medium Gray. Sherwin Williams Polyurethane
Enamel. 11 ounce spray can. Drop Ship item.
VP-902771	Medium Gray. Sherwin Williams Polyurethane
Enamel. 1 quart container. Drop Ship item.
VP-902772	Medium Gray. Sherwin Williams Polyurethane
Enamel. 1 gallon container. Drop Ship item.
VP-902780	Cedar Green. Sherwin Williams Polyurethane
Enamel. 11 ounce spray can. Drop Ship item.
VP-902781	Cedar Green. Sherwin Williams Polyurethane
Enamel. 1 quart container. Drop Ship item.
VP-902782	Cedar Green. Sherwin Williams Polyurethane
Enamel. 1 gallon container. Drop Ship item.
VP-902790	Arctic Blue. Sherwin Williams Polyurethane
Enamel. 11 ounce spray can. Drop Ship item.
VP-902791	Arctic Blue. Sherwin Williams Polyurethane
Enamel. 1 quart container. Drop Ship item.
VP-902792	Arctic Blue. Sherwin Williams Polyurethane
Enamel. 1 gallon container. Drop Ship item.
VP-902801	Clam Chowder. Sherwin Williams Polyurethane
Enamel. 1 quart container. Drop Ship item.
VP-902802	Clam Chowder. Sherwin Williams Polyurethane
Enamel. 1 gallon container. Drop Ship item.
PANS
VP-830145	Drip pan, 10" x 14", 2-1/8" deep. Used under rope
shackles on top of car.
VP-830150	Dust pan, Rubbermaid #2006.
VP-830175	9" paint roller (w/handle) and tray set. 
VP-830210	Drip pan & small bracket for 22CT machine worm
shaft.
VP-830211	Drip pan & large bracket for 29CT machine worm
shaft.

	Page 39

Subject	VP#	Description
PAPER
VP-830350	Fish paper by the sheet. Ideal for protecting motor
fields/armatures. Insulating material. Dupont Nomex #410, 24" x 36" x 20 mil thick.
VP-830400	Red building paper, 500 sq. ft. roll, 3' wide, 20-lb.
paper. Ideal for repair jobs to protect walls and floors.
VP-830410	Waterproof paper, blond laminant, non-staining.
600 sq. ft. roll, 4 ft. wide, approximately 24 lbs. Ideal for floor and wall protection.
PINS
VP-833145	Cotter pin, 1/16" x 1/2", steel with zinc coating
packaged 1,000 pieces/box
VP-833146	Cotter pin 1/16" x 3/4" steel, with zinc coating.
VP-833150	Cotter pin, 3/16" x 1".
VP-833200	Cotter pin, 3/16" x 1-1/2".
VP-833225	Cotter pin, 3/16" x 2".
VP-833300	Cotter pin, 3/16" x 3".
VP-834700	Roll pin, DIN 7346 16 x 36.
VP-834715	Cotter pin, DIN 94 3.2 mm diameter x 20 mm
long.
PIPE PLUGS
VP-836495	1/4" pipe plug, square head. McMaster-Carr
#4468K12. 
VP-836496	Pipe plug, solid, 7/8" O.D.
PLASTIC SHEETS
VP-830420	Floor mask. 24" X 50' roll of hard surface floor
protection. Non-adhesive, non-skid backing. Highly absorbant. Protects from dirt and greases.
VP-830425	Stretch wrap, clear. 15” wide, 1000’ roll. Handles
included on both sides of the roll for easy handling. For use on 2:1 top-to-bottom re-roping jobs. 
VP-830430	Carpet mask. 24" X 200' roll of self-adhesive carpet
protection. Protects from dirt and greases.

	Page 40

Subject	VP#	Description
PLATES PLATES
VP-836100	Safety, brass, maintenance plate.
VP-836101	Safety, chrome, maintenance plate.
PLUGS
VP-836500	Electrical plug, miniature solder type banana plug
Fits miniature 2.64 mm (0.104) dia. banana jack color: black
VP-836501	Electrical plug, miniature solder type banana plug
Fits miniature 2.64 mm (0.104) dia. banana jack color: red
RELAYS
VP-721610	Relay, Allen-Bradley #700P220A24.
VP-840000	Relay # RX120VAC-1.
VP-840015	Relay, Artisan # RB120BAC-1. Used in Otis #4Y‑
6840CK1 assembly.
RESISTORS
VP-840480	Resistor, Ohmite #1744, B12J-2K5, 2500 ohms.
RESPIRATORS
VP-840472	Respirator 6000 series low maintenance type small
size. Mfr. P/N 6100
VP-840473	Respirator 6000 series low maintenance type
medium size. Mfr. P/N 6200
VP-840474	Respirator 6000 series low maintenance type large
size. Mfr. P/N 6300
VP-840485	Respirator cleaning wipes. Box of 100. Individually
packaged. For use with VP-840472, VP-840473, VP-840474. Drop Ship Item.
VP-840487	Respirator storage pouch. High visibility, water
repellent, easy to clean and wear resistant. For use with VP-840472, VP-440473, VP-840474. Drop Ship Item.

Subject	VP#	Description
RESPIRATORS, FILTERS
RESPIRATORS, FILTERS
VP-840490	Filters, respirator. Bag of 2 filters. For all dust,
minerals, organic vapors and acid gas. Use with VP-840472, VP-840473 and VP-840474.
VP-840491	Filters, respirator. Case of 30 bags of 2 filters each.
Organic vapor, acid gas cartridges. For use with VP-840472, VP-840473, and VP-840474.
VP-846309	Dust mask with charcoal overlay. Box of 10.
Includes a laminated "Voluntary Respiratory
Information Card", AAA102ASX1.
RINGS
VP-840709	Axel retaining ring used on UB escalators. 10 DIN
6799. 
RODS
VP-793100	Threaded rod. 3/8" x 16 (UNC thread). 36"
length.
ROLLERS
VP-843581	PVC roller for hoistway doorlock device, Otis # VP‑
843580.
ROPES
VP-843650	7/16" bronze wire rope, 8 x 19 construction. Tail
rope for wedge clamp safety drums.

	Page 42

Subject	VP#	Description
SAFETY SUPPLIES
SAFETY SUPPLIES
VP-754201	No logo safety bag w/ VP#s 773000, 846366,
846355, 846328, 846311, 846387, 754205,
810400, 800211, 704175, 846350, 865050, 810415, and MT-124026-1, MT-114390-1.
VP-754202	Otis logo safety bag w/ VP #'s 773000, 846366,
846345, 846328, 846311, 846387, 754205, 810400, 800209, 704175, 846350, 865050, 810415, and MT-124026-1, MT-114390-1, handbook.
VP-754203-1	Arc Flash PPE Kit Bag, yellow, w/ Otis logo.
vp-754203-2	Arc Flash PPE Kit Bag, yellow, w/o Logo.
VP-754204	GFCI single outlet plug. (Ground Fault Circuit
Interrupter)
VP-754205	GFCI line cord, 2 foot cord length (ground fault
circuit interrupter). Manual resetting. 15A, 120VAC
VP-754210	GFCI line cord, 6 feet cord length. (ground fault
circuit interrupter). Manual resetting. 15A, 120VAC
VP-754215	GFCI line cord, 25 feet cord length, 3 receptacles.
(ground fault circuit interrupter).
VP-754220	GFCI line cord, 50 feet cord length, 3 receptacles.
(ground fault circuit interrupter).
VP-754250	Protective Skin Cream. Protects from most
common skin irritants such as solvents. 2 oz. tube. Drop Ship item.
VP-795085	Arc Flash Barrier. 3’ X 2’ sheet. Meets ASTM F2320
Class 0, Type II, Style B. Yellow, 1,000 volt AC maximum Use, Ozone, Oil and Grease resistant, fire retardant, reinforced.
VP-795090	Arc Flash Barrier. 3’ X 25’ roll. Meets ASTM F2320
Class 0, Type II, Style B. Yellow, 1,000 volt AC maximum Use, Ozone, Oil and Grease resistant, fire retardant, reinforced.
VP-846251	Shade 10 plate. 2" X 4-1/2". Heat treated glass. For
use with welding masks VP-846341 and VP-846326. Drop Ship Item.

	Page 43

Subject	VP#	Description
SAFETY SUPPLIES
VP-846253	Shade 14 plate. 2" X 4-1/2". Heat treated glass. For
use with welding masks VP-846341 and VP-846326. Drop Ship Item.
VP-846255	Clear impact back plate. 2" X 4-1/2". Clear
polycarbonate plate. To be placed under shaded plate. For use with welding masks VP-846341 and VP-846326. Drop Ship Item.
VP-846256	Sleeves, flame retardant cotton protective sleeves.
Protects from above elbow to wrist. 18" long, lightweight. Sold in pairs.
VP-846300	Back support, ATA, size: small
VP-846301	Back support, ATA, size: medium
VP-846302	Back support, ATA, size: large
VP-846303	(Back support), breakaway suspenders size:
adjustable universal fit
VP-846304	Back Support ATA size: extra large
VP-846305	Back support with suspenders, size: XX large.
VP-846310	Safety vest, fluorescent orange.
VP-846316	Goggle case. Heavy duty nylon with zipper and two
belt loops. Drop Ship Item.
VP-846317	Eyewear soft storage case. Ripstop nylon with
draw-string and barrel-lock. Drop Ship Item.
VP-846318	Eyeglass cord. Adjustable, break away cord for
holding safety glasses. Drop Ship Item.
VP-846319	Lens cleaner. Box of pre-moistened towelettes.
Non-silicone based, anti-fog, anti-static,
individually packed tissues to clean glass and plastic lenses. Drop Ship Item.
VP-846320	Face shield attachment for use with hard hat.
Attachment only. Order VP-846322 face shield separately. Drop Ship Item.
VP-846321	Face shield attachment with ratchet adjustment.
Headgear only. Order VP-846322 face shield separately. Drop Ship Item.
VP-846322	Face shield visor replacement. For use with VP‑
846320 and VP-846321. Drop Ship Item.

	Page 44

Subject	VP#	Description
SAFETY SUPPLIES
VP-846323	Glasses, safety, polysafe plus clear. Can be worn
over prescription glasses
VP-846325	UFO Apollo Safety Glasses, clear lens, non-metallic
black frame, adjustable temple length, polycarbonate lens. Drop Ship Item.
VP-846326	Welding goggles. Order plates separately. Drop
Ship Item.
VP-846327	Chemical Goggles, safety. Adjustable venting, soft
PVC frame, anti-fog, anti-static, scratch and impact resistant with UV protection. Drop Ship Item.
VP-846328	Impact Goggles, safety - Vue Guard. With direct
venting, polycarbonate lens material. Drop Ship Item.
VP-846329	Eyeware accessory case. Black, zippered heavy
duty eyeware case. For the storing and
maintaining of eyeware while on jobsites. Drop Ship Item.
VP-846331	Astrospec 3000 safety glasses. Scratch resistant,
anti-fog, clear lens. Black frame with adjustable temples. Drop Ship item.
VP-846332	Astrospec 3001 OTG safety glasses. Fit over most
prescription eyewear. Scratch resistant, anti-fog, clear lens. Black frame with adjustable temples. Drop ship item.
VP-846333	Nassau F6700 safety glasses. Scratch resistant, anti‑
fog, clear lens. Blue frame with adjustable temples. Drop Ship item.
VP-846335	Replacement lens for VP-846331, Astrospec 3000
safety glasses. Scratch resistant, anti-fog, clear lens. Drop Ship item.
VP-846336	Replacement lens for VP-846332, Astro OTG 3001
safety glasses.Scratch resistant, anti-fog, clear lens. Drop Ship item.
VP-846338	Personal Protective Equipment Dispenser. Clear
acrylic, 6-14"H X 12"W X 9"D. Wall or table mount. Can hold safety glasses, ear plugs, dust masks, etc. Drop Ship Item.
VP-846339-1.5	Elvex RX-100 Bifocal Safety Glasses, 1.5 power,
Clear Lens.
VP-846339-2.5	Elvex RX-100 Bifocal Safety Glasses, 2.5 power,
Clear Lens.

	Page 45

Subject	VP#	Description
SAFETY SUPPLIES
VP-846341	Shield, welding. Fiberglass, full-curved, lift front.
Holds 2" X 4-1/2" plates. Use with VP-846342 and VP-846343. Drop Ship Item.
VP-846342	Ratchet headgear for VP-846341 welding shield.
Drop Ship Item.
VP-846343	Hard hat attachment for VP-846341 welding
shield. Non-metallic universal cap adapter, complete with friction joints. Drop Ship Item.
VP-846344	Hard hat rack. Wall mount unit, holds one hard
hat. Drop Ship Item.
VP-846347	Hard hat liner. Flame resistant, two-piece Velcro
closure hood liner, winter weight. No metal parts. Drop Ship Item.
VP-846350	Chin strap, for hard hats. Plastic fasteners attach to
suspension. Drop Ship Item.
VP-846351	Hard hat suspension, sentry III ratchet, 4-point
suspension replacement headgear. Used in VP-846352 through VP-846355. Drop Ship Item.
VP-846352	Hard hat, white with Otis logo. Dialectric with
ratchet suspension, slotted. Adjustable from 6- 1/2" to 8". Drop Ship Item.
VP-846353	Hard hat, yellow with Otis logo. Dialectric with
ratchet suspension, slotted. Adjustable from 6- 1/2" to 8". Drop Ship Item.
VP-846354	Hard hat, white, no logo. Dialectric with ratchet
suspension, slotted. Adjustable from 6-1/2" to 8". Drop Ship Item.
VP-846355	Hard hat, yellow, no logo. Dialectric with ratchet
suspension, slotted. Adjustable from 6-1/2" to 8". Drop Ship Item.
VP-846359	Hard hat sweatband. Terri-cloth band fits to
suspension. Washable, non-metallic. 10 per package. Drop Ship Item.
VP-846360-1	Streamlight rubber helmet/hardhat strap for use
with VP-800231-1 and VP-800231-2.
VP-846367	Lanyard, to fit in every fall protection uniform
listed under base part numbers: VP-846200 through VP-846205 and VP-846370 through VP-846375

	Page 46

Subject	VP#	Description
SAFETY SUPPLIES
VP-846369	Lanyard holster (pouch) 4" x 7.5", expanded
polyester vinyl.
VP-846378	Lanyard, adjustable length w/ shock absorber,
aluminum snap hooks on both ends. For use with fall protection harnesses with D-ring on back.
VP-846379	Lanyard, 100% Tie-Off. Three legs, each having an
aluminum self-locking snap hook. Includes energy absorber in central leg below master link. Suitable for fall protection.
VP-846380	Personal Fall Protection Kit. Includes lanyard, VP‑
846378 and harness w/ D-ring, MT-124040-7.
VP-846381	Microshield rescue breather includes 1-pair of
latex gloves and antiseptic towelettes.
VP-846382	Semi-insert hearing protector. Dielectric headband
with ear pods. Noise reduction rating of 25 dB. Drop Ship Item.
VP-846383	Semi-insert hearing protector replacements.
Package of 5 pair. Use with VP-846382. Drop Ship Item.
VP-846384	Earplugs with storage case. Dielectric. Without
cord. Noise reduction rating of 21dB. Drop Ship Item.
VP-846385	Ear muffs for slotted hard hats. Dielectric. Noise
reduction rating of 23 dB. Use with VP-846345, VP-846346 and VP-846352 through VP-846357. Drop Ship Item.
VP-846386	Ear muffs, dielectric. Noise reduction rating of 22
dB. Drop Ship Item.
VP-846387	Earplugs, reusable, with cord and storage case.
Noise reduction rating of 21 dB. 1 pair. Drop Ship item.
VP-846388	Earplugs, disposable. with cord. Polymer foam.
Noise reduction rating of 29 dB. 200 pair per box. Drop Ship Item.
VP-846389	Earplugs, disposable. Dielectric, polymer foam.
Noise reduction rating of 29 dB. Box of 200 pair. Drop Ship Item.
VP-846390	Carabiner type retrofit Lanyard, without shock
absorber. Adjustable up to 5 ft. in length. Used for retrofit of standard harness/lanyard combinations supplied under VP-846366. 

	Page 47

Subject	VP#	Description
SAFETY SUPPLIES
VP-846398	Bracket for attachment of rail-mounting
retractable lifeline, with mounting hardware. For use only with VP-846399 retractable lifeline. NOT for use with MT-124040.
VP-846399	Lifeline, 30 ft. retractable. For use with VP-846398
mounting bracket. 
VP-846413	Lifeline, self-retracting. Technora web type, 10 ft.
Positive self-locking latch for employee fall protection.
VP-846423	Funnel, safety, with flash arrestor. Used for
storage drums.
VP-846424	Container, fireproof, oily rag.
VP-846425	Zip Lock bags, 100 in a box. Used for waste rag
transfer. 13" x 15".
VP-846428	Lanyard, extension, for fall protection. To ease
attachment of retractable lifeline to harness D-ring.
VP-846435	Kevlar protective sleeve with thumbhole. 18" long
to protect forearm from heavy abrasion. Sold individually.
VP-846440	Knee pads, heavy duty, black, velcro type
fastening, one size fits all.
VP-846445	Red safety dot, for watch faces. Used as a
reminder to "Think Safety". Box of approximately 500 dots.
VP-846450	Duffle bag, for safetyequipment, cordura green
canvas w/Otis logo ingold on both ends of bag, 24 x 14.
VP-846457	Anti-skid warning tape. Grit surfaced black and
yellow striped. 3" wide, 20 yard roll with adhesive backing.
VP-846465	  Edge guard - black, plastic edge trim with adhesive.
	Provides cut and puncture protection from sheet    metal edges up to .125 inches thick. 250 foot roll. 
VP-846466	Edge guard - clear, plastic edge trim with adhesive.
Provides cut and puncture protection from sheet metal edges up to .125 inches thick. 250 foot roll. 
VP-846467	Edge guard - chrome, plastic edge trim with
adhesive. Provides cut and puncture protection from sheet metal edges up to .125 inches thick. 250 foot roll. 

	Page 48

Subject	VP#	Description
SAFETY SUPPLIES
VP-846473	Insoles. Puncture resistant shoe insoles. One Size
Fits All. Complies with ASTM F 2413, OSHA standards for puncture resistance. Not CSA
compliant. Flexible contoured design for comfort.
SAFETY SUPPLIES, FIRE
VP-846417	Fire extinguisher, 20 lb. wall mount, 'ABC' type.
VP-846418	Fire extinguisher, 2.75 lb. vehicle: 'BC' type.
SAFETY SUPPLIES, LABELS
VP-846419	Labels, "Hazardous Waste", 25 in a pack (for
specific chemical identification) 6" x 6" size.
VP-846420	Labels, "NON-Hazardous Waste", 25 in a pack, 6" x
6" size.
VP-846460	Label, Material Identification. Used to identify
materials transferred to secondary containers. Self-adhesive, 1-1/2" X 3-7/8". Drop Ship Item.
VP-846461	Label, Hazard Rating Index. Used to define hazard
ratings and protective equipment needs. Self-adhesive, 4" X 5-7/8". Drop Ship Item.
VP-846462	Label, "DANGER Contains asbestos fibers, avoid
creating dust-cancer and lung disease hazard". Individual label. 3-1/2" x 5".
SAFETY SUPPLIES, SIGNS
VP-846406	10" x 14" rigid plastic sign with "waste storage
area" printed on one side.
VP-846407	7" x 10" door cabinet sign with "danger‑
flammable" printed on one side. Mfr. P/N D126P
VP-846408	10" x 14" wall mount sign with "danger‑
flammable" printed on one side.
VP-846410	9" x 12" "no smoking" sign: vinyl material.
VP-846411	9" x 12" "no smoking" sign: rigid plastic material.
SAFETY SUPPLIES, SPILL
VP-846415	4-drum secondary containment holder.
VP-846416	Single drum secondary containment holder.
VP-846431	Spill response kit. For warehouse type
application.
VP-846432	Vehicle spill response kit, grab and go style.

	Page 49

Subject	VP#	Description
SAFETY SUPPLIES, SPILLS
VP-846433	Refillable vehicle spill response kit. Includes gloves,
a disposal bag, 10 absorbant pads, 2 barrier socks. Enough to contain 5 gallons. Can be refilled with VP-846432 and VP-740100.
SAFETY SUPPLIES, UNIFORMS
VP-714001	Tyvek protective coveralls, hooded. Size large. 6
coveralls per box.
VP-714002	Tyvek protective coveralls, hooded. Size X-large. 6
coveralls per box.
VP-714003	Tyvek protective coveralls, hooded. Size XX-large.
6 coveralls per box.
VP-846200-29	Fall protection bib overall without lanyard. Size
small to fit chest sizes 30-32. Trouser inseam 29". Drop Ship item.
VP-846200-32	Fall protection bib overall without lanyard. Size
small to fit chest sizes 30-32. Trouser inseam 32". Drop Ship item.
VP-846201-29	Fall protection bib overall without lanyard. Size
medium to fit chest sizes 34-36. Trouser inseam 29". Drop Ship item.
VP-846201-32	Fall protection bib overall without lanyard. Size
medium to fit chest sizes 34-36. Trouser inseam 32". Drop Ship item.
VP-846201-35	Fall protection bib overall without lanyard. Size
medium to fit chest sizes 34-36. Trouser inseam 35". Drop Ship item.
VP-846202-29	Fall protection bib overall without lanyard. Size
large to fit chest sizes 38-40. Trouser inseam 29". Drop Ship item.
VP-846202-32	Fall protection bib overall without lanyard. Size
large to fit chest sizes 38-40. Trouser inseam 32". Drop Ship item.
VP-846202-35	Fall protection bib overall without lanyard. Size
large to fit chest sizes 38-40. Trouser inseam 35". Drop Ship item.
VP-846203-29	Fall protection bib overall without lanyard. Size X‑
large to fit chest sizes 42-44. Trouser inseam 29". Drop Ship item.
VP-846203-32	Fall protection bib overall without lanyard. Size X‑
large to fit chest sizes 42-44. Trouser inseam 32". Drop Ship item.

	Page 50

Subject	VP#	Description
SAFETY SUPPLIES, UNIFORMS
VP-846203-35	Fall protection bib overall without lanyard. Size X‑
large to fit chest sizes 42-44. Trouser inseam 35". Drop Ship item.
VP-846204-29	Fall protection bib overall without lanyard. Size XX‑
large to fit chest sizes 46-48. Trouser inseam 29". Drop Ship item.
VP-846204-32	Fall protection bib overall without lanyard. Size XX‑
large to fit chest sizes 46-48. Trouser inseam 32". Drop Ship item.
VP-846204-35	Fall protection bib overall without lanyard. Size XX‑
large to fit chest sizes 46-48. Trouser inseam 35". Drop Ship item.
VP-846205-32	Fall protection bib overall without lanyard. Size
XXX-large to fit chest sizes 50-52. Trouser inseam 32". Drop Ship item.
VP-846205-35	Fall protection bib overall without lanyard. Size
XXX-large to fit chest sizes 50-52. Trouser inseam 35". Drop Ship item.
VP-846371-32LS	Fall protection uniform without lanyard. Size
medium to fit chest sizes 38-41. Trouser inseam 32", long sleeve shirt.

	Page 51

Subject	VP#	Description
SCREWS
SCREWS
VP-846825	10-32 x 3/4" pan head machine screw, steel.
American Std. cadmium plate, yellow iridite, SCMA P10-32x3/4.
VP-846830	Flat head countersunk Phillips screw, 5-40 x 3/8",
electro plated.
VP-846832	#6 x 1/2" flat head, countersunk, Phillips head, self
tapping, black screw.
VP-846835	Flat head countersunk Phillips screw, 6-32 x 3/8",
electro plated.
VP-846840	Round head self tapping screw, #6 x 1/2", electro
plated.
VP-846900	5-40 x 1/4" binding head machine screw,brass.
American Std. cadmium plate, yellow iridite, SCMA BBR5-40x1/4.
VP-849700	4-40 x 1/2" pan head screw, type F, cadmium
plated.
VP-849883	Low head socket cap screw, DIN 7984 M12 x 35.
VP-849884	Stainless steel screw, DIN 7991 M4 x 10.
VP-849885	Slotted pan head machine screw, DIN 84 M6 x 25.
VP-849887	Socket flat head brass screw (countersunk). M4 x
10 DIN # 7991. For escalator decking panels.
VP-849889	Slotted flat head machine screw, DIN 963 M6 x 12.
VP-849890	Phillips flat head machine screw, stainless steel; for
UB escalator molding. DIN 965 M6 x 12.
VP-851010	Socket head cap screw, DIN 912 M10 x 20.
VP-852000	Flat head machine screw, DIN 963 M8 x 25.
VP-855350	5-40 x 3/8" oval head Phillips machine screw,
steel. SCMA OP5-40x3/8.
VP-855355	6-32 x 3/8" flat head Phillips self-tapping screw,
type F, black.
VP-855357	6-32 x 3/8" pan head Phillips sems, ext. lockwasher
machine screw
VP-855358	6-32 X 1/4" pan head screw. Pan Phillips sems,
(w/external lockwasher) zinc plated. Used with 456DD1 roller to make 7593B4 door guide.

	Page 52

Subject	VP#	Description
SCREWS
VP-855360	6-32 x 3/8" flat head sheet metal drive, screw,
type B, black.
VP-855361	Screw Tek #3, sheet metal: hex washer head, #12 X
3/4" long, with a bar seal washer. Zinc plated steel. For sheet metal
VP-855365	Cap screw, hex head 4-40 x 1/2 inch.
VP-855500	10-24 x 1/2" flat head nylon machine screw.
VP-855550	Avsafe tamper resistant screw, # MCRM 1024-
1000. 
VP-855860	8-32 x 1/2 SEMS (external lockwasher, Phillips)
VP-855866	8-32 x 1-1/2" tamper proof screw, stainless steel,
snake eyes.
VP-855876	8-32 x 1-1/2" tamper proof screw, brass, snake
eyes.
VP-860045	10-32 x 3-1/2" pan head machine screw. SCMA
P10-32x3-1/2.
VP-860650	10-32 x 1" oval head Phillips machine screw,
brass.
VP-860660	USE P/N: 124DK33. Spanner oval head machine
screw, Stainless steel, 6-32 x 1", SCMA OCKSPSS6- 32 x 1.
VP-860670	USE P/N: 124DK34. Spanner oval head machine
screw, Brass, 6-32 x 1", SCMA OCKSPBR-32 x 1.
VP-860700	10-32 x 3/4" oval head Phillips recessed machine
screw, stainless steel.
VP-860710	USE P/N: 124DK37. 10-32 x 1" spanner oval head
machine screw, stainless steel. SCMA OCKSPSS10- 32x1.
VP-860720	1/4" x 3/8" machine screw whiz lock type, flanged.
SCMA LKFLG1/4 x 3/8WHIZ.
VP-862420	10 x 1/2" pan head steel Parker Kalon type Z self‑
tapping screw. SCPT PPKZ10x1/2.
VP-862430	TORX tamper-resistant screw. Pan, pin-in-head,
self-drilling screw. Size T25, #10 X 3/4"
VP-863310	1/2"-13x2" Square Head Cone Point Set Screw.
Used with AAA336PV1 Beam Clamp for AAA22242C1 Rerope Service Tool.

	Page 53

Subject	VP#	Description
SEALS
SEALS
VP-864540	Seal for `O' operator, #240731. 1" x 1-1/4" x 1/8".
SHAPES
VP-768300	USE P/N: AAA50ASV. Extrusion shape A. 874
machine conversion. 
VP-768500	USE P/N: AAA50ASZ. Extrusion shape E1. 874
	machine conversion. 
SHIMS
VP-869605	4-1/2" shim, vulcanized fiber, 4-3/8" x 5-3/8" x
1/16" thick. Texacone #2F002-001.
VP-869610	5" shim, vulcanized fiber, 4-7/8" x 5-7/8" x 1/16"
thick. Texacone #2F012-001.
VP-869615	5-1/2" shim, vulcanized fiber, 5-7/16" x 6-7/16" x
1/16" thick. Texacone #2F003-001.
SHOES
VP-869750	Door guide shoe, Adams #0-678. 
SLEEVING
VP-871600	Sleeving Kit for Hydro Motor Lead Sleeving.,
Contains wire lead sleeves, ties, markers and instructions for 6 wire leads. For motors with 12 leads, two kits are needed. 
SOCKETS
VP-872300	Lamp socket, B8200J.
 SPACER
VP-874270	Insulated spacer. A circuit tap consisting of a
phenolic tube internally threaded 8/32; one end w/nut & stud. 

	Page 54

Subject	VP#	Description
SHOES
SPLICERS
VP-749100	But splice, T & B Sta-Kon part # 2RB14X.
VP-749110	In-line insulated splice connector. Wire size range:
14 AWG to 1/0 AWG. Eliminates taping of field connections on motors and generators. 
VP-749111	In-line insulated splice connector. Wire size range:
10 AWG to 250 kcmil. Eliminates taping of field connections on motors and generators. 
VP-749112	In-line insulated splice connector. Wire size range:
10 AWG to 350 kcmil. Eliminates taping of field connections on motors and generators. 
VP-749113	In-line insulated splice connector. Wire size range:
6 AWG to 500 kcmil. Eliminates taping of field connections on motors and generators. 
SPRAYERS
VP-875025	Two-gallon garden type sprayer. Hudson Sprayer
#6215.
VP-875030	12 polyethylene 32 oz. spray bottles w/adjustable
nozzle (sprayer is for use with Simple Green cleaner Otis P/N VP-420480).
SPRINGS
VP-843582	Spring for hoistway door lock device, Otis # VP‑
843580.
VP-876400	Spring, Peelle #03457.
STANDOFFS
VP-877550	8-32, (Externally threaded both ends) brass hex
standoff. Used in 2700ABA1 and VP-874270.
VP-877565	Nylon standoff, 1" x 1/4", 8-32 tapped thru.
VP-877577	Hex standoff for 7770R operator door motor
retrofit kit, VP-798605.
STAPLE REMOVER
VP-877600	Packaging staple remover.
STARTERS
VP-877650	Starter for flourescent lights, FS5.
VP-877700	Starter for flourescent lights, FS25.
VP-877730	Starter for flourescent light fixture 460-78 Vendor: OSRAM (Germany) #ST 151

	Page 55

Subject	VP#	Description
STONES
STONES
VP-878200	Brush seating stone medium grade, 1-1/4" x 2-1/2"
x 4-3/4".
VP-880000	#1 flex stone, coarse, Rimac 80 grit.
VP-880010	#2 flex stone, fine, Rimac 120 grit.
VP-880050	Coarse lathe stone for cleaning commutators. 1" x
2" x 8", grade C.
VP-880100	Fine lathe stone for cleaning commmutators, 1" x
2" x 8", grade F.
STRIKERS
VP-881700	Solid striker used on Otis 311B type hall lantern
gong. 
SUPPRESSORS
VP-882500	Sleeve Ferrite clamp. Used on MRQ VFCU as base
	current oscillation inhibitors. 
SWITCHES
VP-883145	Switch, Micro Switch # BZE6-2RQ62.
TAGS
VP-884600	Lockout safety tag. Rigid vinyl tag w/ 3/8"
grommeted hole. Tag reads "DANGER-Locked to protect workman repairing machinery". Also avail. AAA102AFZ1, self-adhering tag.
TAPES
VP-890700	Pipe sealant tape, 1/2" wide. Used in "Piping Kit
for Hydraulic Elevators", # VP-798460. 
VP-890800	Electrical tape, 3/4" wide, 20-foot roll, black vinyl.
VP-890850	Electrical tape, 3/4" wide, 66-foot roll, black vinyl.

	Page 56

Subject	VP#	Description
TAPES
VP-890855	Electrical tape, 3/4" wide, 66-foot roll, yellow
vinyl. Drop Ship Item.
VP-890980	Scotch tape #472, 6" wide, black.
VP-891300	Friction tape, 3/4" wide, 60-foot roll. Per Federal
Spec. HHT-101A.
VP-891600	Masking tape, 2" wide, 60-yard roll.
VP-891850	Pipe thread sealant tape, 1/2" wide, 43-foot roll.
MIL Spec T-27730A. 3M Co. #48
VP-892500	Teflon tape, 1" wide, 36-yard roll.
VP-892520	Scotch brand filament tape, reinforced with glass
yarn. 1" X 60 yard roll.
TAPS
VP-874270	SEE SPACERS.
VP-885400	1/4-20 UNC plug tap. High speed steel, 4-flutes, 1"
thread length, 3-5 threads chamfered, 2-1/2" overall length, H3 pitch diameter limit
VP-885500	5/16" x 18" standard tap. SEE Circular Letter SS‑
39A-75.
VP-885505	5/16" x 18" bottoming tap.
VP-885510	3-48 tap, 2 flute.
VP-889750	6-32 tap, 2 flute. Union #1534.
VP-889775	8-32 plug tap, 4 flute.
VP-890055	Plug style tap; 3/8"-16 thread; 3 flute; spiral; H3
pitch diameter limits; "GUN" brand for hand or machine tapping. Was P/N REP-TAP2.
VP-890250	1/2-13 tap, 3 flute.
VP-890255	Plug style tap;5/8"-11 thread;4 flute; spiral; H3
pitch diameter limits; GTD/GREENFIELD brand for hand tapping. Was P/N REP-TAP3.
VP-890265	3/4"-10 taper tap, 4 flute. 

	Page 57

Subject	VP#	Description
TERMINALS
TERMINALS
VP-749200	Locking spade terminal. T & B part # RA18-10FL.
Sold in box of 100 pieces
VP-893700	Ring terminal, Thomas & Betts # B14-8.
VP-894001	Ring tongue terminal. Amp P/N: 32945
VP-894028	Ring terminal, Thomas & Betts # B14-14.
VP-894100	Female disconnecting terminal. 18 guage wire,
1/4" x 0.032" tab, vinyl insulated
THERMOSTATS
VP-896660	Thermostat for door operators, used in
conjunction with VP-792553 heater. SEE Dwg. A7300AH, Airpax, Inc./No. American Phillips Controls #5100-003-173
VP-896660	Thermostat for door operators, used in
conjunction with VP-792553 heater. SEE Dwg. A7300AH, Airpax, Inc./No. American Phillips Controls #5100-003-173
TOOL BOXES
VP-898700	Wheeled utility bag for convenient transport of
tools/parts. Extendable axles for increased stability. Removable tool holders, extendable handle, five secondary compartments, and removable small parts box mounted on back.
VP-898701	Metal tool box for examiners. Kennedy style,
cantilever tray professional tool box. Industrial Supplies Company, P/N: CS-16. See also,
alternative polyethylene tool box MT-104001.
WASHERS
VP-904200	Plastic washer, Amatom #2322-N.
VP-904890	DIN 127 A8 steel lock washer.
VP-904892	DIN 127 A12 steel lock washer.
VP-904958	DIN 125 6 steel flat washer.
VP-904960	DIN 125 8 steel flat washer.
VP-904962	DIN 125 10 steel flat washer.
VP-904964	DIN 125 12 steel flat washer.

	Page 58

Subject	VP#	Description
WASHERS
VP-904965	DIN 125 13 steel flat washer.
VP-904979	DIN 127 A6 steel lock washer.
VP-904981	DIN 127 A10 steel lock washer.
VP-904985	DIN 127 A16 steel lock washer.
VP-904989	DIN 434 9 square tapered washer.
VP-905040	DIN 9021 6 oversized flat steel washer.
VP-906200	#8 x 5/32" steel shakeproof lock washer. WSR SP8-
1208. Same as Otis #130A4.
VP-906220	1" steel shakeproof lock washer. WSR SP1-1236.
Same as Otis #130A16.
VP-906800	Cadmium washer, NO10.
VP-908710	5/16" lock washer. SEE Circular Letter SS-39A-75.
VP-908800	3/8" standard "Kantlink" spring lock washer. Same
as Otis #130F9.
VP-908910	1/4" fender washer. 
VP-909100	#10 standard lock washer. WSR LK10.
VP-910950	5/8" Truscon washer. Nut holder for concrete
inserts.
VP-910960	Washer, reducing. From 1" to 3/4". Used on AT400
Generic Retrofit Kits, AAA24430V.
WIPERS
VP-919990	Wiper cloth. Linx cleaning cloth by Prematex. Box
of 1100 wipers in 100 count bags. High durability, absorbancy. Strong and softer than bulk cloth wipers.
VP-920000	Wiper cloth, sweatshirt, Sold per 10 lb. box
VP-920010	Wiper cloth, polo-knIt, 10 lb. box

	Page 59

Subject	VP#	Description
WIRES
VP-749300	Red wire, 22AWG Kynar wire,10 mil insulation.
VP-749301	Wire, 22 AWG , black, 300V, 80°, UL style 1061,
CSA type SR-PVC. Sold by foot
VP-876785	Music wire, .023 x 1/8 O.D., natural finish, close
wound, left-hand wind, Lee Spring Co. # E-023.
VP-912890	USE P/N: AAA800A3. Black annealed wire, 14ga.,
supplied in a 5 lb. spool....which yields approx. 290 feet of wire.
VP-912900	Black soft steel wire, 21 gauge, 1/4-lb.roll.
VP-913350	Music wire, 14 gauge, .032" thick, 5-lb. 1720 foot
spool. Used on types 6339B and 6339C wire drives for #5 floor controller.
VP-913550	Music wire, 21 gauge, .047" thick, 5-lb. 850 foot
spool. Used on types 6339B, 6339D and 6339E wire drives for #5 floor controller.
VP-913650	Plumb wire, 16 gauge (.062" diameter) 12 lb spool.
VP-914600	Black stranded wire, 14 gauge, type THHN/THWN.
VP-915100	Black stranded wire, 16 gauge, type MTW.
VP-915200	Red stranded wire, 18 gauge, type TFF.
VP-916048	White wire, #18AWG, stranded, 600V, 105C, UL
Style1015, CSA TEW 1000 foot reel
VP-916049	Wire, Violet/Yellow, 1000 foot reel, #18 AWG
600V 105C UL style 1015
VP-916051	Grey wire, #18AWG, used in GAMMA D man.,
600V 105C UL style 1015 Manhattan part # M214.
VP-916052	Green & Yellow wire, #18AWG, used in GAMMA D,
600V 105C UL style 1015 Manhattan part # M214.
VP-916053	Black wire, #8AWG, used in GAMMA D man.
VP-916054	Black wire, #14AWG, for GAMMA D man. 600V
105C UL style 1015 Manhattan part # M216.

	Page 60

Subject	VP#	Description
WIRES
VP-916055	Green & Yellow wire, #14AWG, used in GAMMA D,
600V 105C UL style 1015 Manhattan part # M216.
VP-916056	Grey wire, #14AWG, used in GAMMA D man.
600V 105C UL style 1015 Manhattan part # M216.
VP-916060	Black stranded wire, 18AWG, 600V, 105ºC, CSA
TEW, UL style 1015
VP-916061	Green & Yellow wire, #8AWG, used in GAMMA D,
600V 105C UL style 1028 Manhattan part # M219.
VP-916063	Black wire, #18AWG, used in GAMMA D man. For
DOOR RES.
VP-916065	Wire, 10 AWG, black, 600V, 105°C. Vendor:
Belden. Vendor P/N: 9910, color #10.
VP-916066	Wire, 10 AWG, red, 600V, 105°C. Vendor: Belden.
Vendor P/N: 9910, color #2.
VP-916067	Wire, 6 AWG, black, 600V, 150°C. Vendor: Belden.
Vendor P/N: 37106.
VP-916068	Wire, 4 AWG, black, 600V, 150°C. Vendor: Belden.
Vendor P/N: 37104.
VP-916070	Wire, BLUE, #22AWG. Vendor: Belden Wire.
Vendor P/N: 8503
VP-916080	Wire, GREEN, #18AWG. Spec #26.
VP-916083	Wire, 2 pairs 22 AWG overall shield, 300V, 80°C.
Vendor: Belden. Vendor P/N: 9302.
VP-916084	Wire, 6 pairs 22 AWG overall shield, 300V, 80°C.
Vendor: Belden. Vendor P/N: 9306.
VP-916086	Wire, 2 conductor 18 AWG cord SJO-2. 300V,
60°C. Vendor: Belden. Vendor P/N: 19227.
VP-916100	Blue stranded wire, 18 gauge, type TFFN.
VP-917375	Solid PVC style 1007 slate color wire, 22 gauge.
VP-917400	Silicone wire, Spec 28, used for selector wiring and
SCC switches.